MG32F10x Standard Peripherals Firmware Library

core_cm3.h
浏览该文件的文档.
1 /**************************************************************************/
7 /*
8 * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
9 *
10 * SPDX-License-Identifier: Apache-2.0
11 *
12 * Licensed under the Apache License, Version 2.0 (the License); you may
13 * not use this file except in compliance with the License.
14 * You may obtain a copy of the License at
15 *
16 * www.apache.org/licenses/LICENSE-2.0
17 *
18 * Unless required by applicable law or agreed to in writing, software
19 * distributed under the License is distributed on an AS IS BASIS, WITHOUT
20 * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
21 * See the License for the specific language governing permissions and
22 * limitations under the License.
23 */
24
25 #if defined ( __ICCARM__ )
26 #pragma system_include /* treat file as system include file for MISRA check */
27 #elif defined (__clang__)
28 #pragma clang system_header /* treat file as system include file */
29 #endif
30
31 #ifndef __CORE_CM3_H_GENERIC
32 #define __CORE_CM3_H_GENERIC
33
34 #include <stdint.h>
35
36 #ifdef __cplusplus
37 extern "C" {
38 #endif
39
55 /*******************************************************************************
56 * CMSIS definitions
57 ******************************************************************************/
63 #include "cmsis_version.h"
64
65 /* CMSIS CM3 definitions */
66 #define __CM3_CMSIS_VERSION_MAIN (__CM_CMSIS_VERSION_MAIN)
67 #define __CM3_CMSIS_VERSION_SUB (__CM_CMSIS_VERSION_SUB)
68 #define __CM3_CMSIS_VERSION ((__CM3_CMSIS_VERSION_MAIN << 16U) | \
69 __CM3_CMSIS_VERSION_SUB )
71 #define __CORTEX_M (3U)
76 #define __FPU_USED 0U
77
78 #if defined ( __CC_ARM )
79 #if defined __TARGET_FPU_VFP
80 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
81 #endif
82
83 #elif defined (__ARMCC_VERSION) && (__ARMCC_VERSION >= 6010050)
84 #if defined __ARM_PCS_VFP
85 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
86 #endif
87
88 #elif defined ( __GNUC__ )
89 #if defined (__VFP_FP__) && !defined(__SOFTFP__)
90 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
91 #endif
92
93 #elif defined ( __ICCARM__ )
94 #if defined __ARMVFP__
95 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
96 #endif
97
98 #elif defined ( __TI_ARM__ )
99 #if defined __TI_VFP_SUPPORT__
100 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
101 #endif
102
103 #elif defined ( __TASKING__ )
104 #if defined __FPU_VFP__
105 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
106 #endif
107
108 #elif defined ( __CSMC__ )
109 #if ( __CSMC__ & 0x400U)
110 #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)"
111 #endif
112
113 #endif
114
115 #include "cmsis_compiler.h" /* CMSIS compiler specific defines */
116
117
118 #ifdef __cplusplus
119 }
120 #endif
121
122 #endif /* __CORE_CM3_H_GENERIC */
123
124 #ifndef __CMSIS_GENERIC
125
126 #ifndef __CORE_CM3_H_DEPENDANT
127 #define __CORE_CM3_H_DEPENDANT
128
129 #ifdef __cplusplus
130 extern "C" {
131 #endif
132
133 /* check device defines and use defaults */
134 #if defined __CHECK_DEVICE_DEFINES
135 #ifndef __CM3_REV
136 #define __CM3_REV 0x0200U
137 #warning "__CM3_REV not defined in device header file; using default!"
138 #endif
139
140 #ifndef __MPU_PRESENT
141 #define __MPU_PRESENT 0U
142 #warning "__MPU_PRESENT not defined in device header file; using default!"
143 #endif
144
145 #ifndef __NVIC_PRIO_BITS
146 #define __NVIC_PRIO_BITS 3U
147 #warning "__NVIC_PRIO_BITS not defined in device header file; using default!"
148 #endif
149
150 #ifndef __Vendor_SysTickConfig
151 #define __Vendor_SysTickConfig 0U
152 #warning "__Vendor_SysTickConfig not defined in device header file; using default!"
153 #endif
154 #endif
155
156 /* IO definitions (access restrictions to peripheral registers) */
164 #ifdef __cplusplus
165 #define __I volatile
166 #else
167 #define __I volatile const
168 #endif
169 #define __O volatile
170 #define __IO volatile
172 /* following defines should be used for structure members */
173 #define __IM volatile const
174 #define __OM volatile
175 #define __IOM volatile
177
181 /*******************************************************************************
182 * Register Abstraction
183 Core Register contain:
184 - Core Register
185 - Core NVIC Register
186 - Core SCB Register
187 - Core SysTick Register
188 - Core Debug Register
189 - Core MPU Register
190 ******************************************************************************/
191
206 typedef union
207 {
208 struct
209 {
210 uint32_t _reserved0:27;
211 uint32_t Q:1;
212 uint32_t V:1;
213 uint32_t C:1;
214 uint32_t Z:1;
215 uint32_t N:1;
216 } b;
217 uint32_t w;
218 } APSR_Type;
219
220 /* APSR Register Definitions */
221 #define APSR_N_Pos 31U
222 #define APSR_N_Msk (1UL << APSR_N_Pos)
224 #define APSR_Z_Pos 30U
225 #define APSR_Z_Msk (1UL << APSR_Z_Pos)
227 #define APSR_C_Pos 29U
228 #define APSR_C_Msk (1UL << APSR_C_Pos)
230 #define APSR_V_Pos 28U
231 #define APSR_V_Msk (1UL << APSR_V_Pos)
233 #define APSR_Q_Pos 27U
234 #define APSR_Q_Msk (1UL << APSR_Q_Pos)
240 typedef union
241 {
242 struct
243 {
244 uint32_t ISR:9;
245 uint32_t _reserved0:23;
246 } b;
247 uint32_t w;
248 } IPSR_Type;
249
250 /* IPSR Register Definitions */
251 #define IPSR_ISR_Pos 0U
252 #define IPSR_ISR_Msk (0x1FFUL /*<< IPSR_ISR_Pos*/)
258 typedef union
259 {
260 struct
261 {
262 uint32_t ISR:9;
263 uint32_t _reserved0:1;
264 uint32_t ICI_IT_1:6;
265 uint32_t _reserved1:8;
266 uint32_t T:1;
267 uint32_t ICI_IT_2:2;
268 uint32_t Q:1;
269 uint32_t V:1;
270 uint32_t C:1;
271 uint32_t Z:1;
272 uint32_t N:1;
273 } b;
274 uint32_t w;
275 } xPSR_Type;
276
277 /* xPSR Register Definitions */
278 #define xPSR_N_Pos 31U
279 #define xPSR_N_Msk (1UL << xPSR_N_Pos)
281 #define xPSR_Z_Pos 30U
282 #define xPSR_Z_Msk (1UL << xPSR_Z_Pos)
284 #define xPSR_C_Pos 29U
285 #define xPSR_C_Msk (1UL << xPSR_C_Pos)
287 #define xPSR_V_Pos 28U
288 #define xPSR_V_Msk (1UL << xPSR_V_Pos)
290 #define xPSR_Q_Pos 27U
291 #define xPSR_Q_Msk (1UL << xPSR_Q_Pos)
293 #define xPSR_ICI_IT_2_Pos 25U
294 #define xPSR_ICI_IT_2_Msk (3UL << xPSR_ICI_IT_2_Pos)
296 #define xPSR_T_Pos 24U
297 #define xPSR_T_Msk (1UL << xPSR_T_Pos)
299 #define xPSR_ICI_IT_1_Pos 10U
300 #define xPSR_ICI_IT_1_Msk (0x3FUL << xPSR_ICI_IT_1_Pos)
302 #define xPSR_ISR_Pos 0U
303 #define xPSR_ISR_Msk (0x1FFUL /*<< xPSR_ISR_Pos*/)
309 typedef union
310 {
311 struct
312 {
313 uint32_t nPRIV:1;
314 uint32_t SPSEL:1;
315 uint32_t _reserved1:30;
316 } b;
317 uint32_t w;
318 } CONTROL_Type;
319
320 /* CONTROL Register Definitions */
321 #define CONTROL_SPSEL_Pos 1U
322 #define CONTROL_SPSEL_Msk (1UL << CONTROL_SPSEL_Pos)
324 #define CONTROL_nPRIV_Pos 0U
325 #define CONTROL_nPRIV_Msk (1UL /*<< CONTROL_nPRIV_Pos*/)
327
340 typedef struct
341 {
342 __IOM uint32_t ISER[8U];
343 uint32_t RESERVED0[24U];
344 __IOM uint32_t ICER[8U];
345 uint32_t RSERVED1[24U];
346 __IOM uint32_t ISPR[8U];
347 uint32_t RESERVED2[24U];
348 __IOM uint32_t ICPR[8U];
349 uint32_t RESERVED3[24U];
350 __IOM uint32_t IABR[8U];
351 uint32_t RESERVED4[56U];
352 __IOM uint8_t IP[240U];
353 uint32_t RESERVED5[644U];
354 __OM uint32_t STIR;
355 } NVIC_Type;
356
357 /* Software Triggered Interrupt Register Definitions */
358 #define NVIC_STIR_INTID_Pos 0U
359 #define NVIC_STIR_INTID_Msk (0x1FFUL /*<< NVIC_STIR_INTID_Pos*/)
361
374 typedef struct
375 {
376 __IM uint32_t CPUID;
377 __IOM uint32_t ICSR;
378 __IOM uint32_t VTOR;
379 __IOM uint32_t AIRCR;
380 __IOM uint32_t SCR;
381 __IOM uint32_t CCR;
382 __IOM uint8_t SHP[12U];
383 __IOM uint32_t SHCSR;
384 __IOM uint32_t CFSR;
385 __IOM uint32_t HFSR;
386 __IOM uint32_t DFSR;
387 __IOM uint32_t MMFAR;
388 __IOM uint32_t BFAR;
389 __IOM uint32_t AFSR;
390 __IM uint32_t PFR[2U];
391 __IM uint32_t DFR;
392 __IM uint32_t ADR;
393 __IM uint32_t MMFR[4U];
394 __IM uint32_t ISAR[5U];
395 uint32_t RESERVED0[5U];
396 __IOM uint32_t CPACR;
397 } SCB_Type;
398
399 /* SCB CPUID Register Definitions */
400 #define SCB_CPUID_IMPLEMENTER_Pos 24U
401 #define SCB_CPUID_IMPLEMENTER_Msk (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)
403 #define SCB_CPUID_VARIANT_Pos 20U
404 #define SCB_CPUID_VARIANT_Msk (0xFUL << SCB_CPUID_VARIANT_Pos)
406 #define SCB_CPUID_ARCHITECTURE_Pos 16U
407 #define SCB_CPUID_ARCHITECTURE_Msk (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)
409 #define SCB_CPUID_PARTNO_Pos 4U
410 #define SCB_CPUID_PARTNO_Msk (0xFFFUL << SCB_CPUID_PARTNO_Pos)
412 #define SCB_CPUID_REVISION_Pos 0U
413 #define SCB_CPUID_REVISION_Msk (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)
415 /* SCB Interrupt Control State Register Definitions */
416 #define SCB_ICSR_NMIPENDSET_Pos 31U
417 #define SCB_ICSR_NMIPENDSET_Msk (1UL << SCB_ICSR_NMIPENDSET_Pos)
419 #define SCB_ICSR_PENDSVSET_Pos 28U
420 #define SCB_ICSR_PENDSVSET_Msk (1UL << SCB_ICSR_PENDSVSET_Pos)
422 #define SCB_ICSR_PENDSVCLR_Pos 27U
423 #define SCB_ICSR_PENDSVCLR_Msk (1UL << SCB_ICSR_PENDSVCLR_Pos)
425 #define SCB_ICSR_PENDSTSET_Pos 26U
426 #define SCB_ICSR_PENDSTSET_Msk (1UL << SCB_ICSR_PENDSTSET_Pos)
428 #define SCB_ICSR_PENDSTCLR_Pos 25U
429 #define SCB_ICSR_PENDSTCLR_Msk (1UL << SCB_ICSR_PENDSTCLR_Pos)
431 #define SCB_ICSR_ISRPREEMPT_Pos 23U
432 #define SCB_ICSR_ISRPREEMPT_Msk (1UL << SCB_ICSR_ISRPREEMPT_Pos)
434 #define SCB_ICSR_ISRPENDING_Pos 22U
435 #define SCB_ICSR_ISRPENDING_Msk (1UL << SCB_ICSR_ISRPENDING_Pos)
437 #define SCB_ICSR_VECTPENDING_Pos 12U
438 #define SCB_ICSR_VECTPENDING_Msk (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)
440 #define SCB_ICSR_RETTOBASE_Pos 11U
441 #define SCB_ICSR_RETTOBASE_Msk (1UL << SCB_ICSR_RETTOBASE_Pos)
443 #define SCB_ICSR_VECTACTIVE_Pos 0U
444 #define SCB_ICSR_VECTACTIVE_Msk (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)
446 /* SCB Vector Table Offset Register Definitions */
447 #if defined (__CM3_REV) && (__CM3_REV < 0x0201U) /* core r2p1 */
448 #define SCB_VTOR_TBLBASE_Pos 29U
449 #define SCB_VTOR_TBLBASE_Msk (1UL << SCB_VTOR_TBLBASE_Pos)
451 #define SCB_VTOR_TBLOFF_Pos 7U
452 #define SCB_VTOR_TBLOFF_Msk (0x3FFFFFUL << SCB_VTOR_TBLOFF_Pos)
453 #else
454 #define SCB_VTOR_TBLOFF_Pos 7U
455 #define SCB_VTOR_TBLOFF_Msk (0x1FFFFFFUL << SCB_VTOR_TBLOFF_Pos)
456 #endif
457
458 /* SCB Application Interrupt and Reset Control Register Definitions */
459 #define SCB_AIRCR_VECTKEY_Pos 16U
460 #define SCB_AIRCR_VECTKEY_Msk (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)
462 #define SCB_AIRCR_VECTKEYSTAT_Pos 16U
463 #define SCB_AIRCR_VECTKEYSTAT_Msk (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)
465 #define SCB_AIRCR_ENDIANESS_Pos 15U
466 #define SCB_AIRCR_ENDIANESS_Msk (1UL << SCB_AIRCR_ENDIANESS_Pos)
468 #define SCB_AIRCR_PRIGROUP_Pos 8U
469 #define SCB_AIRCR_PRIGROUP_Msk (7UL << SCB_AIRCR_PRIGROUP_Pos)
471 #define SCB_AIRCR_SYSRESETREQ_Pos 2U
472 #define SCB_AIRCR_SYSRESETREQ_Msk (1UL << SCB_AIRCR_SYSRESETREQ_Pos)
474 #define SCB_AIRCR_VECTCLRACTIVE_Pos 1U
475 #define SCB_AIRCR_VECTCLRACTIVE_Msk (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)
477 #define SCB_AIRCR_VECTRESET_Pos 0U
478 #define SCB_AIRCR_VECTRESET_Msk (1UL /*<< SCB_AIRCR_VECTRESET_Pos*/)
480 /* SCB System Control Register Definitions */
481 #define SCB_SCR_SEVONPEND_Pos 4U
482 #define SCB_SCR_SEVONPEND_Msk (1UL << SCB_SCR_SEVONPEND_Pos)
484 #define SCB_SCR_SLEEPDEEP_Pos 2U
485 #define SCB_SCR_SLEEPDEEP_Msk (1UL << SCB_SCR_SLEEPDEEP_Pos)
487 #define SCB_SCR_SLEEPONEXIT_Pos 1U
488 #define SCB_SCR_SLEEPONEXIT_Msk (1UL << SCB_SCR_SLEEPONEXIT_Pos)
490 /* SCB Configuration Control Register Definitions */
491 #define SCB_CCR_STKALIGN_Pos 9U
492 #define SCB_CCR_STKALIGN_Msk (1UL << SCB_CCR_STKALIGN_Pos)
494 #define SCB_CCR_BFHFNMIGN_Pos 8U
495 #define SCB_CCR_BFHFNMIGN_Msk (1UL << SCB_CCR_BFHFNMIGN_Pos)
497 #define SCB_CCR_DIV_0_TRP_Pos 4U
498 #define SCB_CCR_DIV_0_TRP_Msk (1UL << SCB_CCR_DIV_0_TRP_Pos)
500 #define SCB_CCR_UNALIGN_TRP_Pos 3U
501 #define SCB_CCR_UNALIGN_TRP_Msk (1UL << SCB_CCR_UNALIGN_TRP_Pos)
503 #define SCB_CCR_USERSETMPEND_Pos 1U
504 #define SCB_CCR_USERSETMPEND_Msk (1UL << SCB_CCR_USERSETMPEND_Pos)
506 #define SCB_CCR_NONBASETHRDENA_Pos 0U
507 #define SCB_CCR_NONBASETHRDENA_Msk (1UL /*<< SCB_CCR_NONBASETHRDENA_Pos*/)
509 /* SCB System Handler Control and State Register Definitions */
510 #define SCB_SHCSR_USGFAULTENA_Pos 18U
511 #define SCB_SHCSR_USGFAULTENA_Msk (1UL << SCB_SHCSR_USGFAULTENA_Pos)
513 #define SCB_SHCSR_BUSFAULTENA_Pos 17U
514 #define SCB_SHCSR_BUSFAULTENA_Msk (1UL << SCB_SHCSR_BUSFAULTENA_Pos)
516 #define SCB_SHCSR_MEMFAULTENA_Pos 16U
517 #define SCB_SHCSR_MEMFAULTENA_Msk (1UL << SCB_SHCSR_MEMFAULTENA_Pos)
519 #define SCB_SHCSR_SVCALLPENDED_Pos 15U
520 #define SCB_SHCSR_SVCALLPENDED_Msk (1UL << SCB_SHCSR_SVCALLPENDED_Pos)
522 #define SCB_SHCSR_BUSFAULTPENDED_Pos 14U
523 #define SCB_SHCSR_BUSFAULTPENDED_Msk (1UL << SCB_SHCSR_BUSFAULTPENDED_Pos)
525 #define SCB_SHCSR_MEMFAULTPENDED_Pos 13U
526 #define SCB_SHCSR_MEMFAULTPENDED_Msk (1UL << SCB_SHCSR_MEMFAULTPENDED_Pos)
528 #define SCB_SHCSR_USGFAULTPENDED_Pos 12U
529 #define SCB_SHCSR_USGFAULTPENDED_Msk (1UL << SCB_SHCSR_USGFAULTPENDED_Pos)
531 #define SCB_SHCSR_SYSTICKACT_Pos 11U
532 #define SCB_SHCSR_SYSTICKACT_Msk (1UL << SCB_SHCSR_SYSTICKACT_Pos)
534 #define SCB_SHCSR_PENDSVACT_Pos 10U
535 #define SCB_SHCSR_PENDSVACT_Msk (1UL << SCB_SHCSR_PENDSVACT_Pos)
537 #define SCB_SHCSR_MONITORACT_Pos 8U
538 #define SCB_SHCSR_MONITORACT_Msk (1UL << SCB_SHCSR_MONITORACT_Pos)
540 #define SCB_SHCSR_SVCALLACT_Pos 7U
541 #define SCB_SHCSR_SVCALLACT_Msk (1UL << SCB_SHCSR_SVCALLACT_Pos)
543 #define SCB_SHCSR_USGFAULTACT_Pos 3U
544 #define SCB_SHCSR_USGFAULTACT_Msk (1UL << SCB_SHCSR_USGFAULTACT_Pos)
546 #define SCB_SHCSR_BUSFAULTACT_Pos 1U
547 #define SCB_SHCSR_BUSFAULTACT_Msk (1UL << SCB_SHCSR_BUSFAULTACT_Pos)
549 #define SCB_SHCSR_MEMFAULTACT_Pos 0U
550 #define SCB_SHCSR_MEMFAULTACT_Msk (1UL /*<< SCB_SHCSR_MEMFAULTACT_Pos*/)
552 /* SCB Configurable Fault Status Register Definitions */
553 #define SCB_CFSR_USGFAULTSR_Pos 16U
554 #define SCB_CFSR_USGFAULTSR_Msk (0xFFFFUL << SCB_CFSR_USGFAULTSR_Pos)
556 #define SCB_CFSR_BUSFAULTSR_Pos 8U
557 #define SCB_CFSR_BUSFAULTSR_Msk (0xFFUL << SCB_CFSR_BUSFAULTSR_Pos)
559 #define SCB_CFSR_MEMFAULTSR_Pos 0U
560 #define SCB_CFSR_MEMFAULTSR_Msk (0xFFUL /*<< SCB_CFSR_MEMFAULTSR_Pos*/)
562 /* MemManage Fault Status Register (part of SCB Configurable Fault Status Register) */
563 #define SCB_CFSR_MMARVALID_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 7U)
564 #define SCB_CFSR_MMARVALID_Msk (1UL << SCB_CFSR_MMARVALID_Pos)
566 #define SCB_CFSR_MSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 4U)
567 #define SCB_CFSR_MSTKERR_Msk (1UL << SCB_CFSR_MSTKERR_Pos)
569 #define SCB_CFSR_MUNSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 3U)
570 #define SCB_CFSR_MUNSTKERR_Msk (1UL << SCB_CFSR_MUNSTKERR_Pos)
572 #define SCB_CFSR_DACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 1U)
573 #define SCB_CFSR_DACCVIOL_Msk (1UL << SCB_CFSR_DACCVIOL_Pos)
575 #define SCB_CFSR_IACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 0U)
576 #define SCB_CFSR_IACCVIOL_Msk (1UL /*<< SCB_CFSR_IACCVIOL_Pos*/)
578 /* BusFault Status Register (part of SCB Configurable Fault Status Register) */
579 #define SCB_CFSR_BFARVALID_Pos (SCB_CFSR_BUSFAULTSR_Pos + 7U)
580 #define SCB_CFSR_BFARVALID_Msk (1UL << SCB_CFSR_BFARVALID_Pos)
582 #define SCB_CFSR_STKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 4U)
583 #define SCB_CFSR_STKERR_Msk (1UL << SCB_CFSR_STKERR_Pos)
585 #define SCB_CFSR_UNSTKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 3U)
586 #define SCB_CFSR_UNSTKERR_Msk (1UL << SCB_CFSR_UNSTKERR_Pos)
588 #define SCB_CFSR_IMPRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 2U)
589 #define SCB_CFSR_IMPRECISERR_Msk (1UL << SCB_CFSR_IMPRECISERR_Pos)
591 #define SCB_CFSR_PRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 1U)
592 #define SCB_CFSR_PRECISERR_Msk (1UL << SCB_CFSR_PRECISERR_Pos)
594 #define SCB_CFSR_IBUSERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 0U)
595 #define SCB_CFSR_IBUSERR_Msk (1UL << SCB_CFSR_IBUSERR_Pos)
597 /* UsageFault Status Register (part of SCB Configurable Fault Status Register) */
598 #define SCB_CFSR_DIVBYZERO_Pos (SCB_CFSR_USGFAULTSR_Pos + 9U)
599 #define SCB_CFSR_DIVBYZERO_Msk (1UL << SCB_CFSR_DIVBYZERO_Pos)
601 #define SCB_CFSR_UNALIGNED_Pos (SCB_CFSR_USGFAULTSR_Pos + 8U)
602 #define SCB_CFSR_UNALIGNED_Msk (1UL << SCB_CFSR_UNALIGNED_Pos)
604 #define SCB_CFSR_NOCP_Pos (SCB_CFSR_USGFAULTSR_Pos + 3U)
605 #define SCB_CFSR_NOCP_Msk (1UL << SCB_CFSR_NOCP_Pos)
607 #define SCB_CFSR_INVPC_Pos (SCB_CFSR_USGFAULTSR_Pos + 2U)
608 #define SCB_CFSR_INVPC_Msk (1UL << SCB_CFSR_INVPC_Pos)
610 #define SCB_CFSR_INVSTATE_Pos (SCB_CFSR_USGFAULTSR_Pos + 1U)
611 #define SCB_CFSR_INVSTATE_Msk (1UL << SCB_CFSR_INVSTATE_Pos)
613 #define SCB_CFSR_UNDEFINSTR_Pos (SCB_CFSR_USGFAULTSR_Pos + 0U)
614 #define SCB_CFSR_UNDEFINSTR_Msk (1UL << SCB_CFSR_UNDEFINSTR_Pos)
616 /* SCB Hard Fault Status Register Definitions */
617 #define SCB_HFSR_DEBUGEVT_Pos 31U
618 #define SCB_HFSR_DEBUGEVT_Msk (1UL << SCB_HFSR_DEBUGEVT_Pos)
620 #define SCB_HFSR_FORCED_Pos 30U
621 #define SCB_HFSR_FORCED_Msk (1UL << SCB_HFSR_FORCED_Pos)
623 #define SCB_HFSR_VECTTBL_Pos 1U
624 #define SCB_HFSR_VECTTBL_Msk (1UL << SCB_HFSR_VECTTBL_Pos)
626 /* SCB Debug Fault Status Register Definitions */
627 #define SCB_DFSR_EXTERNAL_Pos 4U
628 #define SCB_DFSR_EXTERNAL_Msk (1UL << SCB_DFSR_EXTERNAL_Pos)
630 #define SCB_DFSR_VCATCH_Pos 3U
631 #define SCB_DFSR_VCATCH_Msk (1UL << SCB_DFSR_VCATCH_Pos)
633 #define SCB_DFSR_DWTTRAP_Pos 2U
634 #define SCB_DFSR_DWTTRAP_Msk (1UL << SCB_DFSR_DWTTRAP_Pos)
636 #define SCB_DFSR_BKPT_Pos 1U
637 #define SCB_DFSR_BKPT_Msk (1UL << SCB_DFSR_BKPT_Pos)
639 #define SCB_DFSR_HALTED_Pos 0U
640 #define SCB_DFSR_HALTED_Msk (1UL /*<< SCB_DFSR_HALTED_Pos*/)
642
655 typedef struct
656 {
657 uint32_t RESERVED0[1U];
658 __IM uint32_t ICTR;
659 #if defined (__CM3_REV) && (__CM3_REV >= 0x200U)
660 __IOM uint32_t ACTLR;
661 #else
662 uint32_t RESERVED1[1U];
663 #endif
664 } SCnSCB_Type;
665
666 /* Interrupt Controller Type Register Definitions */
667 #define SCnSCB_ICTR_INTLINESNUM_Pos 0U
668 #define SCnSCB_ICTR_INTLINESNUM_Msk (0xFUL /*<< SCnSCB_ICTR_INTLINESNUM_Pos*/)
670 /* Auxiliary Control Register Definitions */
671
672 #define SCnSCB_ACTLR_DISFOLD_Pos 2U
673 #define SCnSCB_ACTLR_DISFOLD_Msk (1UL << SCnSCB_ACTLR_DISFOLD_Pos)
675 #define SCnSCB_ACTLR_DISDEFWBUF_Pos 1U
676 #define SCnSCB_ACTLR_DISDEFWBUF_Msk (1UL << SCnSCB_ACTLR_DISDEFWBUF_Pos)
678 #define SCnSCB_ACTLR_DISMCYCINT_Pos 0U
679 #define SCnSCB_ACTLR_DISMCYCINT_Msk (1UL /*<< SCnSCB_ACTLR_DISMCYCINT_Pos*/)
681
694 typedef struct
695 {
696 __IOM uint32_t CTRL;
697 __IOM uint32_t LOAD;
698 __IOM uint32_t VAL;
699 __IM uint32_t CALIB;
700 } SysTick_Type;
701
702 /* SysTick Control / Status Register Definitions */
703 #define SysTick_CTRL_COUNTFLAG_Pos 16U
704 #define SysTick_CTRL_COUNTFLAG_Msk (1UL << SysTick_CTRL_COUNTFLAG_Pos)
706 #define SysTick_CTRL_CLKSOURCE_Pos 2U
707 #define SysTick_CTRL_CLKSOURCE_Msk (1UL << SysTick_CTRL_CLKSOURCE_Pos)
709 #define SysTick_CTRL_TICKINT_Pos 1U
710 #define SysTick_CTRL_TICKINT_Msk (1UL << SysTick_CTRL_TICKINT_Pos)
712 #define SysTick_CTRL_ENABLE_Pos 0U
713 #define SysTick_CTRL_ENABLE_Msk (1UL /*<< SysTick_CTRL_ENABLE_Pos*/)
715 /* SysTick Reload Register Definitions */
716 #define SysTick_LOAD_RELOAD_Pos 0U
717 #define SysTick_LOAD_RELOAD_Msk (0xFFFFFFUL /*<< SysTick_LOAD_RELOAD_Pos*/)
719 /* SysTick Current Register Definitions */
720 #define SysTick_VAL_CURRENT_Pos 0U
721 #define SysTick_VAL_CURRENT_Msk (0xFFFFFFUL /*<< SysTick_VAL_CURRENT_Pos*/)
723 /* SysTick Calibration Register Definitions */
724 #define SysTick_CALIB_NOREF_Pos 31U
725 #define SysTick_CALIB_NOREF_Msk (1UL << SysTick_CALIB_NOREF_Pos)
727 #define SysTick_CALIB_SKEW_Pos 30U
728 #define SysTick_CALIB_SKEW_Msk (1UL << SysTick_CALIB_SKEW_Pos)
730 #define SysTick_CALIB_TENMS_Pos 0U
731 #define SysTick_CALIB_TENMS_Msk (0xFFFFFFUL /*<< SysTick_CALIB_TENMS_Pos*/)
733
746 typedef struct
747 {
748 __OM union
749 {
750 __OM uint8_t u8;
751 __OM uint16_t u16;
752 __OM uint32_t u32;
753 } PORT [32U];
754 uint32_t RESERVED0[864U];
755 __IOM uint32_t TER;
756 uint32_t RESERVED1[15U];
757 __IOM uint32_t TPR;
758 uint32_t RESERVED2[15U];
759 __IOM uint32_t TCR;
760 uint32_t RESERVED3[29U];
761 __OM uint32_t IWR;
762 __IM uint32_t IRR;
763 __IOM uint32_t IMCR;
764 uint32_t RESERVED4[43U];
765 __OM uint32_t LAR;
766 __IM uint32_t LSR;
767 uint32_t RESERVED5[6U];
768 __IM uint32_t PID4;
769 __IM uint32_t PID5;
770 __IM uint32_t PID6;
771 __IM uint32_t PID7;
772 __IM uint32_t PID0;
773 __IM uint32_t PID1;
774 __IM uint32_t PID2;
775 __IM uint32_t PID3;
776 __IM uint32_t CID0;
777 __IM uint32_t CID1;
778 __IM uint32_t CID2;
779 __IM uint32_t CID3;
780 } ITM_Type;
781
782 /* ITM Trace Privilege Register Definitions */
783 #define ITM_TPR_PRIVMASK_Pos 0U
784 #define ITM_TPR_PRIVMASK_Msk (0xFFFFFFFFUL /*<< ITM_TPR_PRIVMASK_Pos*/)
786 /* ITM Trace Control Register Definitions */
787 #define ITM_TCR_BUSY_Pos 23U
788 #define ITM_TCR_BUSY_Msk (1UL << ITM_TCR_BUSY_Pos)
790 #define ITM_TCR_TraceBusID_Pos 16U
791 #define ITM_TCR_TraceBusID_Msk (0x7FUL << ITM_TCR_TraceBusID_Pos)
793 #define ITM_TCR_GTSFREQ_Pos 10U
794 #define ITM_TCR_GTSFREQ_Msk (3UL << ITM_TCR_GTSFREQ_Pos)
796 #define ITM_TCR_TSPrescale_Pos 8U
797 #define ITM_TCR_TSPrescale_Msk (3UL << ITM_TCR_TSPrescale_Pos)
799 #define ITM_TCR_SWOENA_Pos 4U
800 #define ITM_TCR_SWOENA_Msk (1UL << ITM_TCR_SWOENA_Pos)
802 #define ITM_TCR_DWTENA_Pos 3U
803 #define ITM_TCR_DWTENA_Msk (1UL << ITM_TCR_DWTENA_Pos)
805 #define ITM_TCR_SYNCENA_Pos 2U
806 #define ITM_TCR_SYNCENA_Msk (1UL << ITM_TCR_SYNCENA_Pos)
808 #define ITM_TCR_TSENA_Pos 1U
809 #define ITM_TCR_TSENA_Msk (1UL << ITM_TCR_TSENA_Pos)
811 #define ITM_TCR_ITMENA_Pos 0U
812 #define ITM_TCR_ITMENA_Msk (1UL /*<< ITM_TCR_ITMENA_Pos*/)
814 /* ITM Integration Write Register Definitions */
815 #define ITM_IWR_ATVALIDM_Pos 0U
816 #define ITM_IWR_ATVALIDM_Msk (1UL /*<< ITM_IWR_ATVALIDM_Pos*/)
818 /* ITM Integration Read Register Definitions */
819 #define ITM_IRR_ATREADYM_Pos 0U
820 #define ITM_IRR_ATREADYM_Msk (1UL /*<< ITM_IRR_ATREADYM_Pos*/)
822 /* ITM Integration Mode Control Register Definitions */
823 #define ITM_IMCR_INTEGRATION_Pos 0U
824 #define ITM_IMCR_INTEGRATION_Msk (1UL /*<< ITM_IMCR_INTEGRATION_Pos*/)
826 /* ITM Lock Status Register Definitions */
827 #define ITM_LSR_ByteAcc_Pos 2U
828 #define ITM_LSR_ByteAcc_Msk (1UL << ITM_LSR_ByteAcc_Pos)
830 #define ITM_LSR_Access_Pos 1U
831 #define ITM_LSR_Access_Msk (1UL << ITM_LSR_Access_Pos)
833 #define ITM_LSR_Present_Pos 0U
834 #define ITM_LSR_Present_Msk (1UL /*<< ITM_LSR_Present_Pos*/)
836 /* end of group CMSIS_ITM */
837
838
849 typedef struct
850 {
851 __IOM uint32_t CTRL;
852 __IOM uint32_t CYCCNT;
853 __IOM uint32_t CPICNT;
854 __IOM uint32_t EXCCNT;
855 __IOM uint32_t SLEEPCNT;
856 __IOM uint32_t LSUCNT;
857 __IOM uint32_t FOLDCNT;
858 __IM uint32_t PCSR;
859 __IOM uint32_t COMP0;
860 __IOM uint32_t MASK0;
861 __IOM uint32_t FUNCTION0;
862 uint32_t RESERVED0[1U];
863 __IOM uint32_t COMP1;
864 __IOM uint32_t MASK1;
865 __IOM uint32_t FUNCTION1;
866 uint32_t RESERVED1[1U];
867 __IOM uint32_t COMP2;
868 __IOM uint32_t MASK2;
869 __IOM uint32_t FUNCTION2;
870 uint32_t RESERVED2[1U];
871 __IOM uint32_t COMP3;
872 __IOM uint32_t MASK3;
873 __IOM uint32_t FUNCTION3;
874 } DWT_Type;
875
876 /* DWT Control Register Definitions */
877 #define DWT_CTRL_NUMCOMP_Pos 28U
878 #define DWT_CTRL_NUMCOMP_Msk (0xFUL << DWT_CTRL_NUMCOMP_Pos)
880 #define DWT_CTRL_NOTRCPKT_Pos 27U
881 #define DWT_CTRL_NOTRCPKT_Msk (0x1UL << DWT_CTRL_NOTRCPKT_Pos)
883 #define DWT_CTRL_NOEXTTRIG_Pos 26U
884 #define DWT_CTRL_NOEXTTRIG_Msk (0x1UL << DWT_CTRL_NOEXTTRIG_Pos)
886 #define DWT_CTRL_NOCYCCNT_Pos 25U
887 #define DWT_CTRL_NOCYCCNT_Msk (0x1UL << DWT_CTRL_NOCYCCNT_Pos)
889 #define DWT_CTRL_NOPRFCNT_Pos 24U
890 #define DWT_CTRL_NOPRFCNT_Msk (0x1UL << DWT_CTRL_NOPRFCNT_Pos)
892 #define DWT_CTRL_CYCEVTENA_Pos 22U
893 #define DWT_CTRL_CYCEVTENA_Msk (0x1UL << DWT_CTRL_CYCEVTENA_Pos)
895 #define DWT_CTRL_FOLDEVTENA_Pos 21U
896 #define DWT_CTRL_FOLDEVTENA_Msk (0x1UL << DWT_CTRL_FOLDEVTENA_Pos)
898 #define DWT_CTRL_LSUEVTENA_Pos 20U
899 #define DWT_CTRL_LSUEVTENA_Msk (0x1UL << DWT_CTRL_LSUEVTENA_Pos)
901 #define DWT_CTRL_SLEEPEVTENA_Pos 19U
902 #define DWT_CTRL_SLEEPEVTENA_Msk (0x1UL << DWT_CTRL_SLEEPEVTENA_Pos)
904 #define DWT_CTRL_EXCEVTENA_Pos 18U
905 #define DWT_CTRL_EXCEVTENA_Msk (0x1UL << DWT_CTRL_EXCEVTENA_Pos)
907 #define DWT_CTRL_CPIEVTENA_Pos 17U
908 #define DWT_CTRL_CPIEVTENA_Msk (0x1UL << DWT_CTRL_CPIEVTENA_Pos)
910 #define DWT_CTRL_EXCTRCENA_Pos 16U
911 #define DWT_CTRL_EXCTRCENA_Msk (0x1UL << DWT_CTRL_EXCTRCENA_Pos)
913 #define DWT_CTRL_PCSAMPLENA_Pos 12U
914 #define DWT_CTRL_PCSAMPLENA_Msk (0x1UL << DWT_CTRL_PCSAMPLENA_Pos)
916 #define DWT_CTRL_SYNCTAP_Pos 10U
917 #define DWT_CTRL_SYNCTAP_Msk (0x3UL << DWT_CTRL_SYNCTAP_Pos)
919 #define DWT_CTRL_CYCTAP_Pos 9U
920 #define DWT_CTRL_CYCTAP_Msk (0x1UL << DWT_CTRL_CYCTAP_Pos)
922 #define DWT_CTRL_POSTINIT_Pos 5U
923 #define DWT_CTRL_POSTINIT_Msk (0xFUL << DWT_CTRL_POSTINIT_Pos)
925 #define DWT_CTRL_POSTPRESET_Pos 1U
926 #define DWT_CTRL_POSTPRESET_Msk (0xFUL << DWT_CTRL_POSTPRESET_Pos)
928 #define DWT_CTRL_CYCCNTENA_Pos 0U
929 #define DWT_CTRL_CYCCNTENA_Msk (0x1UL /*<< DWT_CTRL_CYCCNTENA_Pos*/)
931 /* DWT CPI Count Register Definitions */
932 #define DWT_CPICNT_CPICNT_Pos 0U
933 #define DWT_CPICNT_CPICNT_Msk (0xFFUL /*<< DWT_CPICNT_CPICNT_Pos*/)
935 /* DWT Exception Overhead Count Register Definitions */
936 #define DWT_EXCCNT_EXCCNT_Pos 0U
937 #define DWT_EXCCNT_EXCCNT_Msk (0xFFUL /*<< DWT_EXCCNT_EXCCNT_Pos*/)
939 /* DWT Sleep Count Register Definitions */
940 #define DWT_SLEEPCNT_SLEEPCNT_Pos 0U
941 #define DWT_SLEEPCNT_SLEEPCNT_Msk (0xFFUL /*<< DWT_SLEEPCNT_SLEEPCNT_Pos*/)
943 /* DWT LSU Count Register Definitions */
944 #define DWT_LSUCNT_LSUCNT_Pos 0U
945 #define DWT_LSUCNT_LSUCNT_Msk (0xFFUL /*<< DWT_LSUCNT_LSUCNT_Pos*/)
947 /* DWT Folded-instruction Count Register Definitions */
948 #define DWT_FOLDCNT_FOLDCNT_Pos 0U
949 #define DWT_FOLDCNT_FOLDCNT_Msk (0xFFUL /*<< DWT_FOLDCNT_FOLDCNT_Pos*/)
951 /* DWT Comparator Mask Register Definitions */
952 #define DWT_MASK_MASK_Pos 0U
953 #define DWT_MASK_MASK_Msk (0x1FUL /*<< DWT_MASK_MASK_Pos*/)
955 /* DWT Comparator Function Register Definitions */
956 #define DWT_FUNCTION_MATCHED_Pos 24U
957 #define DWT_FUNCTION_MATCHED_Msk (0x1UL << DWT_FUNCTION_MATCHED_Pos)
959 #define DWT_FUNCTION_DATAVADDR1_Pos 16U
960 #define DWT_FUNCTION_DATAVADDR1_Msk (0xFUL << DWT_FUNCTION_DATAVADDR1_Pos)
962 #define DWT_FUNCTION_DATAVADDR0_Pos 12U
963 #define DWT_FUNCTION_DATAVADDR0_Msk (0xFUL << DWT_FUNCTION_DATAVADDR0_Pos)
965 #define DWT_FUNCTION_DATAVSIZE_Pos 10U
966 #define DWT_FUNCTION_DATAVSIZE_Msk (0x3UL << DWT_FUNCTION_DATAVSIZE_Pos)
968 #define DWT_FUNCTION_LNK1ENA_Pos 9U
969 #define DWT_FUNCTION_LNK1ENA_Msk (0x1UL << DWT_FUNCTION_LNK1ENA_Pos)
971 #define DWT_FUNCTION_DATAVMATCH_Pos 8U
972 #define DWT_FUNCTION_DATAVMATCH_Msk (0x1UL << DWT_FUNCTION_DATAVMATCH_Pos)
974 #define DWT_FUNCTION_CYCMATCH_Pos 7U
975 #define DWT_FUNCTION_CYCMATCH_Msk (0x1UL << DWT_FUNCTION_CYCMATCH_Pos)
977 #define DWT_FUNCTION_EMITRANGE_Pos 5U
978 #define DWT_FUNCTION_EMITRANGE_Msk (0x1UL << DWT_FUNCTION_EMITRANGE_Pos)
980 #define DWT_FUNCTION_FUNCTION_Pos 0U
981 #define DWT_FUNCTION_FUNCTION_Msk (0xFUL /*<< DWT_FUNCTION_FUNCTION_Pos*/)
983 /* end of group CMSIS_DWT */
984
985
996 typedef struct
997 {
998 __IM uint32_t SSPSR;
999 __IOM uint32_t CSPSR;
1000 uint32_t RESERVED0[2U];
1001 __IOM uint32_t ACPR;
1002 uint32_t RESERVED1[55U];
1003 __IOM uint32_t SPPR;
1004 uint32_t RESERVED2[131U];
1005 __IM uint32_t FFSR;
1006 __IOM uint32_t FFCR;
1007 __IM uint32_t FSCR;
1008 uint32_t RESERVED3[759U];
1009 __IM uint32_t TRIGGER;
1010 __IM uint32_t FIFO0;
1011 __IM uint32_t ITATBCTR2;
1012 uint32_t RESERVED4[1U];
1013 __IM uint32_t ITATBCTR0;
1014 __IM uint32_t FIFO1;
1015 __IOM uint32_t ITCTRL;
1016 uint32_t RESERVED5[39U];
1017 __IOM uint32_t CLAIMSET;
1018 __IOM uint32_t CLAIMCLR;
1019 uint32_t RESERVED7[8U];
1020 __IM uint32_t DEVID;
1021 __IM uint32_t DEVTYPE;
1022 } TPI_Type;
1023
1024 /* TPI Asynchronous Clock Prescaler Register Definitions */
1025 #define TPI_ACPR_PRESCALER_Pos 0U
1026 #define TPI_ACPR_PRESCALER_Msk (0x1FFFUL /*<< TPI_ACPR_PRESCALER_Pos*/)
1028 /* TPI Selected Pin Protocol Register Definitions */
1029 #define TPI_SPPR_TXMODE_Pos 0U
1030 #define TPI_SPPR_TXMODE_Msk (0x3UL /*<< TPI_SPPR_TXMODE_Pos*/)
1032 /* TPI Formatter and Flush Status Register Definitions */
1033 #define TPI_FFSR_FtNonStop_Pos 3U
1034 #define TPI_FFSR_FtNonStop_Msk (0x1UL << TPI_FFSR_FtNonStop_Pos)
1036 #define TPI_FFSR_TCPresent_Pos 2U
1037 #define TPI_FFSR_TCPresent_Msk (0x1UL << TPI_FFSR_TCPresent_Pos)
1039 #define TPI_FFSR_FtStopped_Pos 1U
1040 #define TPI_FFSR_FtStopped_Msk (0x1UL << TPI_FFSR_FtStopped_Pos)
1042 #define TPI_FFSR_FlInProg_Pos 0U
1043 #define TPI_FFSR_FlInProg_Msk (0x1UL /*<< TPI_FFSR_FlInProg_Pos*/)
1045 /* TPI Formatter and Flush Control Register Definitions */
1046 #define TPI_FFCR_TrigIn_Pos 8U
1047 #define TPI_FFCR_TrigIn_Msk (0x1UL << TPI_FFCR_TrigIn_Pos)
1049 #define TPI_FFCR_EnFCont_Pos 1U
1050 #define TPI_FFCR_EnFCont_Msk (0x1UL << TPI_FFCR_EnFCont_Pos)
1052 /* TPI TRIGGER Register Definitions */
1053 #define TPI_TRIGGER_TRIGGER_Pos 0U
1054 #define TPI_TRIGGER_TRIGGER_Msk (0x1UL /*<< TPI_TRIGGER_TRIGGER_Pos*/)
1056 /* TPI Integration ETM Data Register Definitions (FIFO0) */
1057 #define TPI_FIFO0_ITM_ATVALID_Pos 29U
1058 #define TPI_FIFO0_ITM_ATVALID_Msk (0x3UL << TPI_FIFO0_ITM_ATVALID_Pos)
1060 #define TPI_FIFO0_ITM_bytecount_Pos 27U
1061 #define TPI_FIFO0_ITM_bytecount_Msk (0x3UL << TPI_FIFO0_ITM_bytecount_Pos)
1063 #define TPI_FIFO0_ETM_ATVALID_Pos 26U
1064 #define TPI_FIFO0_ETM_ATVALID_Msk (0x3UL << TPI_FIFO0_ETM_ATVALID_Pos)
1066 #define TPI_FIFO0_ETM_bytecount_Pos 24U
1067 #define TPI_FIFO0_ETM_bytecount_Msk (0x3UL << TPI_FIFO0_ETM_bytecount_Pos)
1069 #define TPI_FIFO0_ETM2_Pos 16U
1070 #define TPI_FIFO0_ETM2_Msk (0xFFUL << TPI_FIFO0_ETM2_Pos)
1072 #define TPI_FIFO0_ETM1_Pos 8U
1073 #define TPI_FIFO0_ETM1_Msk (0xFFUL << TPI_FIFO0_ETM1_Pos)
1075 #define TPI_FIFO0_ETM0_Pos 0U
1076 #define TPI_FIFO0_ETM0_Msk (0xFFUL /*<< TPI_FIFO0_ETM0_Pos*/)
1078 /* TPI ITATBCTR2 Register Definitions */
1079 #define TPI_ITATBCTR2_ATREADY2_Pos 0U
1080 #define TPI_ITATBCTR2_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY2_Pos*/)
1082 #define TPI_ITATBCTR2_ATREADY1_Pos 0U
1083 #define TPI_ITATBCTR2_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY1_Pos*/)
1085 /* TPI Integration ITM Data Register Definitions (FIFO1) */
1086 #define TPI_FIFO1_ITM_ATVALID_Pos 29U
1087 #define TPI_FIFO1_ITM_ATVALID_Msk (0x3UL << TPI_FIFO1_ITM_ATVALID_Pos)
1089 #define TPI_FIFO1_ITM_bytecount_Pos 27U
1090 #define TPI_FIFO1_ITM_bytecount_Msk (0x3UL << TPI_FIFO1_ITM_bytecount_Pos)
1092 #define TPI_FIFO1_ETM_ATVALID_Pos 26U
1093 #define TPI_FIFO1_ETM_ATVALID_Msk (0x3UL << TPI_FIFO1_ETM_ATVALID_Pos)
1095 #define TPI_FIFO1_ETM_bytecount_Pos 24U
1096 #define TPI_FIFO1_ETM_bytecount_Msk (0x3UL << TPI_FIFO1_ETM_bytecount_Pos)
1098 #define TPI_FIFO1_ITM2_Pos 16U
1099 #define TPI_FIFO1_ITM2_Msk (0xFFUL << TPI_FIFO1_ITM2_Pos)
1101 #define TPI_FIFO1_ITM1_Pos 8U
1102 #define TPI_FIFO1_ITM1_Msk (0xFFUL << TPI_FIFO1_ITM1_Pos)
1104 #define TPI_FIFO1_ITM0_Pos 0U
1105 #define TPI_FIFO1_ITM0_Msk (0xFFUL /*<< TPI_FIFO1_ITM0_Pos*/)
1107 /* TPI ITATBCTR0 Register Definitions */
1108 #define TPI_ITATBCTR0_ATREADY2_Pos 0U
1109 #define TPI_ITATBCTR0_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY2_Pos*/)
1111 #define TPI_ITATBCTR0_ATREADY1_Pos 0U
1112 #define TPI_ITATBCTR0_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY1_Pos*/)
1114 /* TPI Integration Mode Control Register Definitions */
1115 #define TPI_ITCTRL_Mode_Pos 0U
1116 #define TPI_ITCTRL_Mode_Msk (0x3UL /*<< TPI_ITCTRL_Mode_Pos*/)
1118 /* TPI DEVID Register Definitions */
1119 #define TPI_DEVID_NRZVALID_Pos 11U
1120 #define TPI_DEVID_NRZVALID_Msk (0x1UL << TPI_DEVID_NRZVALID_Pos)
1122 #define TPI_DEVID_MANCVALID_Pos 10U
1123 #define TPI_DEVID_MANCVALID_Msk (0x1UL << TPI_DEVID_MANCVALID_Pos)
1125 #define TPI_DEVID_PTINVALID_Pos 9U
1126 #define TPI_DEVID_PTINVALID_Msk (0x1UL << TPI_DEVID_PTINVALID_Pos)
1128 #define TPI_DEVID_MinBufSz_Pos 6U
1129 #define TPI_DEVID_MinBufSz_Msk (0x7UL << TPI_DEVID_MinBufSz_Pos)
1131 #define TPI_DEVID_AsynClkIn_Pos 5U
1132 #define TPI_DEVID_AsynClkIn_Msk (0x1UL << TPI_DEVID_AsynClkIn_Pos)
1134 #define TPI_DEVID_NrTraceInput_Pos 0U
1135 #define TPI_DEVID_NrTraceInput_Msk (0x1FUL /*<< TPI_DEVID_NrTraceInput_Pos*/)
1137 /* TPI DEVTYPE Register Definitions */
1138 #define TPI_DEVTYPE_SubType_Pos 4U
1139 #define TPI_DEVTYPE_SubType_Msk (0xFUL /*<< TPI_DEVTYPE_SubType_Pos*/)
1141 #define TPI_DEVTYPE_MajorType_Pos 0U
1142 #define TPI_DEVTYPE_MajorType_Msk (0xFUL << TPI_DEVTYPE_MajorType_Pos)
1144 /* end of group CMSIS_TPI */
1145
1146
1147 #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1148
1158 typedef struct
1159 {
1160 __IM uint32_t TYPE;
1161 __IOM uint32_t CTRL;
1162 __IOM uint32_t RNR;
1163 __IOM uint32_t RBAR;
1164 __IOM uint32_t RASR;
1165 __IOM uint32_t RBAR_A1;
1166 __IOM uint32_t RASR_A1;
1167 __IOM uint32_t RBAR_A2;
1168 __IOM uint32_t RASR_A2;
1169 __IOM uint32_t RBAR_A3;
1170 __IOM uint32_t RASR_A3;
1171 } MPU_Type;
1172
1173 #define MPU_TYPE_RALIASES 4U
1174
1175 /* MPU Type Register Definitions */
1176 #define MPU_TYPE_IREGION_Pos 16U
1177 #define MPU_TYPE_IREGION_Msk (0xFFUL << MPU_TYPE_IREGION_Pos)
1179 #define MPU_TYPE_DREGION_Pos 8U
1180 #define MPU_TYPE_DREGION_Msk (0xFFUL << MPU_TYPE_DREGION_Pos)
1182 #define MPU_TYPE_SEPARATE_Pos 0U
1183 #define MPU_TYPE_SEPARATE_Msk (1UL /*<< MPU_TYPE_SEPARATE_Pos*/)
1185 /* MPU Control Register Definitions */
1186 #define MPU_CTRL_PRIVDEFENA_Pos 2U
1187 #define MPU_CTRL_PRIVDEFENA_Msk (1UL << MPU_CTRL_PRIVDEFENA_Pos)
1189 #define MPU_CTRL_HFNMIENA_Pos 1U
1190 #define MPU_CTRL_HFNMIENA_Msk (1UL << MPU_CTRL_HFNMIENA_Pos)
1192 #define MPU_CTRL_ENABLE_Pos 0U
1193 #define MPU_CTRL_ENABLE_Msk (1UL /*<< MPU_CTRL_ENABLE_Pos*/)
1195 /* MPU Region Number Register Definitions */
1196 #define MPU_RNR_REGION_Pos 0U
1197 #define MPU_RNR_REGION_Msk (0xFFUL /*<< MPU_RNR_REGION_Pos*/)
1199 /* MPU Region Base Address Register Definitions */
1200 #define MPU_RBAR_ADDR_Pos 5U
1201 #define MPU_RBAR_ADDR_Msk (0x7FFFFFFUL << MPU_RBAR_ADDR_Pos)
1203 #define MPU_RBAR_VALID_Pos 4U
1204 #define MPU_RBAR_VALID_Msk (1UL << MPU_RBAR_VALID_Pos)
1206 #define MPU_RBAR_REGION_Pos 0U
1207 #define MPU_RBAR_REGION_Msk (0xFUL /*<< MPU_RBAR_REGION_Pos*/)
1209 /* MPU Region Attribute and Size Register Definitions */
1210 #define MPU_RASR_ATTRS_Pos 16U
1211 #define MPU_RASR_ATTRS_Msk (0xFFFFUL << MPU_RASR_ATTRS_Pos)
1213 #define MPU_RASR_XN_Pos 28U
1214 #define MPU_RASR_XN_Msk (1UL << MPU_RASR_XN_Pos)
1216 #define MPU_RASR_AP_Pos 24U
1217 #define MPU_RASR_AP_Msk (0x7UL << MPU_RASR_AP_Pos)
1219 #define MPU_RASR_TEX_Pos 19U
1220 #define MPU_RASR_TEX_Msk (0x7UL << MPU_RASR_TEX_Pos)
1222 #define MPU_RASR_S_Pos 18U
1223 #define MPU_RASR_S_Msk (1UL << MPU_RASR_S_Pos)
1225 #define MPU_RASR_C_Pos 17U
1226 #define MPU_RASR_C_Msk (1UL << MPU_RASR_C_Pos)
1228 #define MPU_RASR_B_Pos 16U
1229 #define MPU_RASR_B_Msk (1UL << MPU_RASR_B_Pos)
1231 #define MPU_RASR_SRD_Pos 8U
1232 #define MPU_RASR_SRD_Msk (0xFFUL << MPU_RASR_SRD_Pos)
1234 #define MPU_RASR_SIZE_Pos 1U
1235 #define MPU_RASR_SIZE_Msk (0x1FUL << MPU_RASR_SIZE_Pos)
1237 #define MPU_RASR_ENABLE_Pos 0U
1238 #define MPU_RASR_ENABLE_Msk (1UL /*<< MPU_RASR_ENABLE_Pos*/)
1240
1241 #endif
1242
1243
1254 typedef struct
1255 {
1256 __IOM uint32_t DHCSR;
1257 __OM uint32_t DCRSR;
1258 __IOM uint32_t DCRDR;
1259 __IOM uint32_t DEMCR;
1260 } CoreDebug_Type;
1261
1262 /* Debug Halting Control and Status Register Definitions */
1263 #define CoreDebug_DHCSR_DBGKEY_Pos 16U
1264 #define CoreDebug_DHCSR_DBGKEY_Msk (0xFFFFUL << CoreDebug_DHCSR_DBGKEY_Pos)
1266 #define CoreDebug_DHCSR_S_RESET_ST_Pos 25U
1267 #define CoreDebug_DHCSR_S_RESET_ST_Msk (1UL << CoreDebug_DHCSR_S_RESET_ST_Pos)
1269 #define CoreDebug_DHCSR_S_RETIRE_ST_Pos 24U
1270 #define CoreDebug_DHCSR_S_RETIRE_ST_Msk (1UL << CoreDebug_DHCSR_S_RETIRE_ST_Pos)
1272 #define CoreDebug_DHCSR_S_LOCKUP_Pos 19U
1273 #define CoreDebug_DHCSR_S_LOCKUP_Msk (1UL << CoreDebug_DHCSR_S_LOCKUP_Pos)
1275 #define CoreDebug_DHCSR_S_SLEEP_Pos 18U
1276 #define CoreDebug_DHCSR_S_SLEEP_Msk (1UL << CoreDebug_DHCSR_S_SLEEP_Pos)
1278 #define CoreDebug_DHCSR_S_HALT_Pos 17U
1279 #define CoreDebug_DHCSR_S_HALT_Msk (1UL << CoreDebug_DHCSR_S_HALT_Pos)
1281 #define CoreDebug_DHCSR_S_REGRDY_Pos 16U
1282 #define CoreDebug_DHCSR_S_REGRDY_Msk (1UL << CoreDebug_DHCSR_S_REGRDY_Pos)
1284 #define CoreDebug_DHCSR_C_SNAPSTALL_Pos 5U
1285 #define CoreDebug_DHCSR_C_SNAPSTALL_Msk (1UL << CoreDebug_DHCSR_C_SNAPSTALL_Pos)
1287 #define CoreDebug_DHCSR_C_MASKINTS_Pos 3U
1288 #define CoreDebug_DHCSR_C_MASKINTS_Msk (1UL << CoreDebug_DHCSR_C_MASKINTS_Pos)
1290 #define CoreDebug_DHCSR_C_STEP_Pos 2U
1291 #define CoreDebug_DHCSR_C_STEP_Msk (1UL << CoreDebug_DHCSR_C_STEP_Pos)
1293 #define CoreDebug_DHCSR_C_HALT_Pos 1U
1294 #define CoreDebug_DHCSR_C_HALT_Msk (1UL << CoreDebug_DHCSR_C_HALT_Pos)
1296 #define CoreDebug_DHCSR_C_DEBUGEN_Pos 0U
1297 #define CoreDebug_DHCSR_C_DEBUGEN_Msk (1UL /*<< CoreDebug_DHCSR_C_DEBUGEN_Pos*/)
1299 /* Debug Core Register Selector Register Definitions */
1300 #define CoreDebug_DCRSR_REGWnR_Pos 16U
1301 #define CoreDebug_DCRSR_REGWnR_Msk (1UL << CoreDebug_DCRSR_REGWnR_Pos)
1303 #define CoreDebug_DCRSR_REGSEL_Pos 0U
1304 #define CoreDebug_DCRSR_REGSEL_Msk (0x1FUL /*<< CoreDebug_DCRSR_REGSEL_Pos*/)
1306 /* Debug Exception and Monitor Control Register Definitions */
1307 #define CoreDebug_DEMCR_TRCENA_Pos 24U
1308 #define CoreDebug_DEMCR_TRCENA_Msk (1UL << CoreDebug_DEMCR_TRCENA_Pos)
1310 #define CoreDebug_DEMCR_MON_REQ_Pos 19U
1311 #define CoreDebug_DEMCR_MON_REQ_Msk (1UL << CoreDebug_DEMCR_MON_REQ_Pos)
1313 #define CoreDebug_DEMCR_MON_STEP_Pos 18U
1314 #define CoreDebug_DEMCR_MON_STEP_Msk (1UL << CoreDebug_DEMCR_MON_STEP_Pos)
1316 #define CoreDebug_DEMCR_MON_PEND_Pos 17U
1317 #define CoreDebug_DEMCR_MON_PEND_Msk (1UL << CoreDebug_DEMCR_MON_PEND_Pos)
1319 #define CoreDebug_DEMCR_MON_EN_Pos 16U
1320 #define CoreDebug_DEMCR_MON_EN_Msk (1UL << CoreDebug_DEMCR_MON_EN_Pos)
1322 #define CoreDebug_DEMCR_VC_HARDERR_Pos 10U
1323 #define CoreDebug_DEMCR_VC_HARDERR_Msk (1UL << CoreDebug_DEMCR_VC_HARDERR_Pos)
1325 #define CoreDebug_DEMCR_VC_INTERR_Pos 9U
1326 #define CoreDebug_DEMCR_VC_INTERR_Msk (1UL << CoreDebug_DEMCR_VC_INTERR_Pos)
1328 #define CoreDebug_DEMCR_VC_BUSERR_Pos 8U
1329 #define CoreDebug_DEMCR_VC_BUSERR_Msk (1UL << CoreDebug_DEMCR_VC_BUSERR_Pos)
1331 #define CoreDebug_DEMCR_VC_STATERR_Pos 7U
1332 #define CoreDebug_DEMCR_VC_STATERR_Msk (1UL << CoreDebug_DEMCR_VC_STATERR_Pos)
1334 #define CoreDebug_DEMCR_VC_CHKERR_Pos 6U
1335 #define CoreDebug_DEMCR_VC_CHKERR_Msk (1UL << CoreDebug_DEMCR_VC_CHKERR_Pos)
1337 #define CoreDebug_DEMCR_VC_NOCPERR_Pos 5U
1338 #define CoreDebug_DEMCR_VC_NOCPERR_Msk (1UL << CoreDebug_DEMCR_VC_NOCPERR_Pos)
1340 #define CoreDebug_DEMCR_VC_MMERR_Pos 4U
1341 #define CoreDebug_DEMCR_VC_MMERR_Msk (1UL << CoreDebug_DEMCR_VC_MMERR_Pos)
1343 #define CoreDebug_DEMCR_VC_CORERESET_Pos 0U
1344 #define CoreDebug_DEMCR_VC_CORERESET_Msk (1UL /*<< CoreDebug_DEMCR_VC_CORERESET_Pos*/)
1346
1362 #define _VAL2FLD(field, value) (((uint32_t)(value) << field ## _Pos) & field ## _Msk)
1363
1370 #define _FLD2VAL(field, value) (((uint32_t)(value) & field ## _Msk) >> field ## _Pos)
1371
1382 /* Memory mapping of Core Hardware */
1383 #define SCS_BASE (0xE000E000UL)
1384 #define ITM_BASE (0xE0000000UL)
1385 #define DWT_BASE (0xE0001000UL)
1386 #define TPI_BASE (0xE0040000UL)
1387 #define CoreDebug_BASE (0xE000EDF0UL)
1388 #define SysTick_BASE (SCS_BASE + 0x0010UL)
1389 #define NVIC_BASE (SCS_BASE + 0x0100UL)
1390 #define SCB_BASE (SCS_BASE + 0x0D00UL)
1392 #define SCnSCB ((SCnSCB_Type *) SCS_BASE )
1393 #define SCB ((SCB_Type *) SCB_BASE )
1394 #define SysTick ((SysTick_Type *) SysTick_BASE )
1395 #define NVIC ((NVIC_Type *) NVIC_BASE )
1396 #define ITM ((ITM_Type *) ITM_BASE )
1397 #define DWT ((DWT_Type *) DWT_BASE )
1398 #define TPI ((TPI_Type *) TPI_BASE )
1399 #define CoreDebug ((CoreDebug_Type *) CoreDebug_BASE)
1401 #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1402 #define MPU_BASE (SCS_BASE + 0x0D90UL)
1403 #define MPU ((MPU_Type *) MPU_BASE )
1404 #endif
1405
1410 /*******************************************************************************
1411 * Hardware Abstraction Layer
1412 Core Function Interface contains:
1413 - Core NVIC Functions
1414 - Core SysTick Functions
1415 - Core Debug Functions
1416 - Core Register Access Functions
1417 ******************************************************************************/
1424 /* ########################## NVIC functions #################################### */
1432 #ifdef CMSIS_NVIC_VIRTUAL
1433 #ifndef CMSIS_NVIC_VIRTUAL_HEADER_FILE
1434 #define CMSIS_NVIC_VIRTUAL_HEADER_FILE "cmsis_nvic_virtual.h"
1435 #endif
1436 #include CMSIS_NVIC_VIRTUAL_HEADER_FILE
1437 #else
1438 #define NVIC_SetPriorityGrouping __NVIC_SetPriorityGrouping
1439 #define NVIC_GetPriorityGrouping __NVIC_GetPriorityGrouping
1440 #define NVIC_EnableIRQ __NVIC_EnableIRQ
1441 #define NVIC_GetEnableIRQ __NVIC_GetEnableIRQ
1442 #define NVIC_DisableIRQ __NVIC_DisableIRQ
1443 #define NVIC_GetPendingIRQ __NVIC_GetPendingIRQ
1444 #define NVIC_SetPendingIRQ __NVIC_SetPendingIRQ
1445 #define NVIC_ClearPendingIRQ __NVIC_ClearPendingIRQ
1446 #define NVIC_GetActive __NVIC_GetActive
1447 #define NVIC_SetPriority __NVIC_SetPriority
1448 #define NVIC_GetPriority __NVIC_GetPriority
1449 #define NVIC_SystemReset __NVIC_SystemReset
1450 #endif /* CMSIS_NVIC_VIRTUAL */
1451
1452 #ifdef CMSIS_VECTAB_VIRTUAL
1453 #ifndef CMSIS_VECTAB_VIRTUAL_HEADER_FILE
1454 #define CMSIS_VECTAB_VIRTUAL_HEADER_FILE "cmsis_vectab_virtual.h"
1455 #endif
1456 #include CMSIS_VECTAB_VIRTUAL_HEADER_FILE
1457 #else
1458 #define NVIC_SetVector __NVIC_SetVector
1459 #define NVIC_GetVector __NVIC_GetVector
1460 #endif /* (CMSIS_VECTAB_VIRTUAL) */
1461
1462 #define NVIC_USER_IRQ_OFFSET 16
1463
1464
1465 /* The following EXC_RETURN values are saved the LR on exception entry */
1466 #define EXC_RETURN_HANDLER (0xFFFFFFF1UL) /* return to Handler mode, uses MSP after return */
1467 #define EXC_RETURN_THREAD_MSP (0xFFFFFFF9UL) /* return to Thread mode, uses MSP after return */
1468 #define EXC_RETURN_THREAD_PSP (0xFFFFFFFDUL) /* return to Thread mode, uses PSP after return */
1469
1470
1480 __STATIC_INLINE void __NVIC_SetPriorityGrouping(uint32_t PriorityGroup)
1481 {
1482 uint32_t reg_value;
1483 uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL); /* only values 0..7 are used */
1484
1485 reg_value = SCB->AIRCR; /* read old register configuration */
1486 reg_value &= ~((uint32_t)(SCB_AIRCR_VECTKEY_Msk | SCB_AIRCR_PRIGROUP_Msk)); /* clear bits to change */
1487 reg_value = (reg_value |
1488 ((uint32_t)0x5FAUL << SCB_AIRCR_VECTKEY_Pos) |
1489 (PriorityGroupTmp << SCB_AIRCR_PRIGROUP_Pos) ); /* Insert write key and priority group */
1490 SCB->AIRCR = reg_value;
1491 }
1492
1493
1499 __STATIC_INLINE uint32_t __NVIC_GetPriorityGrouping(void)
1500 {
1501 return ((uint32_t)((SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) >> SCB_AIRCR_PRIGROUP_Pos));
1502 }
1503
1504
1511 __STATIC_INLINE void __NVIC_EnableIRQ(IRQn_Type IRQn)
1512 {
1513 if ((int32_t)(IRQn) >= 0)
1514 {
1515 NVIC->ISER[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1516 }
1517 }
1518
1519
1528 __STATIC_INLINE uint32_t __NVIC_GetEnableIRQ(IRQn_Type IRQn)
1529 {
1530 if ((int32_t)(IRQn) >= 0)
1531 {
1532 return((uint32_t)(((NVIC->ISER[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL))) != 0UL) ? 1UL : 0UL));
1533 }
1534 else
1535 {
1536 return(0U);
1537 }
1538 }
1539
1540
1547 __STATIC_INLINE void __NVIC_DisableIRQ(IRQn_Type IRQn)
1548 {
1549 if ((int32_t)(IRQn) >= 0)
1550 {
1551 NVIC->ICER[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1552 __DSB();
1553 __ISB();
1554 }
1555 }
1556
1557
1566 __STATIC_INLINE uint32_t __NVIC_GetPendingIRQ(IRQn_Type IRQn)
1567 {
1568 if ((int32_t)(IRQn) >= 0)
1569 {
1570 return((uint32_t)(((NVIC->ISPR[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL))) != 0UL) ? 1UL : 0UL));
1571 }
1572 else
1573 {
1574 return(0U);
1575 }
1576 }
1577
1578
1585 __STATIC_INLINE void __NVIC_SetPendingIRQ(IRQn_Type IRQn)
1586 {
1587 if ((int32_t)(IRQn) >= 0)
1588 {
1589 NVIC->ISPR[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1590 }
1591 }
1592
1593
1600 __STATIC_INLINE void __NVIC_ClearPendingIRQ(IRQn_Type IRQn)
1601 {
1602 if ((int32_t)(IRQn) >= 0)
1603 {
1604 NVIC->ICPR[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1605 }
1606 }
1607
1608
1617 __STATIC_INLINE uint32_t __NVIC_GetActive(IRQn_Type IRQn)
1618 {
1619 if ((int32_t)(IRQn) >= 0)
1620 {
1621 return((uint32_t)(((NVIC->IABR[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL))) != 0UL) ? 1UL : 0UL));
1622 }
1623 else
1624 {
1625 return(0U);
1626 }
1627 }
1628
1629
1639 __STATIC_INLINE void __NVIC_SetPriority(IRQn_Type IRQn, uint32_t priority)
1640 {
1641 if ((int32_t)(IRQn) >= 0)
1642 {
1643 NVIC->IP[((uint32_t)IRQn)] = (uint8_t)((priority << (8U - __NVIC_PRIO_BITS)) & (uint32_t)0xFFUL);
1644 }
1645 else
1646 {
1647 SCB->SHP[(((uint32_t)IRQn) & 0xFUL)-4UL] = (uint8_t)((priority << (8U - __NVIC_PRIO_BITS)) & (uint32_t)0xFFUL);
1648 }
1649 }
1650
1651
1661 __STATIC_INLINE uint32_t __NVIC_GetPriority(IRQn_Type IRQn)
1662 {
1663
1664 if ((int32_t)(IRQn) >= 0)
1665 {
1666 return(((uint32_t)NVIC->IP[((uint32_t)IRQn)] >> (8U - __NVIC_PRIO_BITS)));
1667 }
1668 else
1669 {
1670 return(((uint32_t)SCB->SHP[(((uint32_t)IRQn) & 0xFUL)-4UL] >> (8U - __NVIC_PRIO_BITS)));
1671 }
1672 }
1673
1674
1686 __STATIC_INLINE uint32_t NVIC_EncodePriority (uint32_t PriorityGroup, uint32_t PreemptPriority, uint32_t SubPriority)
1687 {
1688 uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL); /* only values 0..7 are used */
1689 uint32_t PreemptPriorityBits;
1690 uint32_t SubPriorityBits;
1691
1692 PreemptPriorityBits = ((7UL - PriorityGroupTmp) > (uint32_t)(__NVIC_PRIO_BITS)) ? (uint32_t)(__NVIC_PRIO_BITS) : (uint32_t)(7UL - PriorityGroupTmp);
1693 SubPriorityBits = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint32_t)0UL : (uint32_t)((PriorityGroupTmp - 7UL) + (uint32_t)(__NVIC_PRIO_BITS));
1694
1695 return (
1696 ((PreemptPriority & (uint32_t)((1UL << (PreemptPriorityBits)) - 1UL)) << SubPriorityBits) |
1697 ((SubPriority & (uint32_t)((1UL << (SubPriorityBits )) - 1UL)))
1698 );
1699 }
1700
1701
1713 __STATIC_INLINE void NVIC_DecodePriority (uint32_t Priority, uint32_t PriorityGroup, uint32_t* const pPreemptPriority, uint32_t* const pSubPriority)
1714 {
1715 uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL); /* only values 0..7 are used */
1716 uint32_t PreemptPriorityBits;
1717 uint32_t SubPriorityBits;
1718
1719 PreemptPriorityBits = ((7UL - PriorityGroupTmp) > (uint32_t)(__NVIC_PRIO_BITS)) ? (uint32_t)(__NVIC_PRIO_BITS) : (uint32_t)(7UL - PriorityGroupTmp);
1720 SubPriorityBits = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint32_t)0UL : (uint32_t)((PriorityGroupTmp - 7UL) + (uint32_t)(__NVIC_PRIO_BITS));
1721
1722 *pPreemptPriority = (Priority >> SubPriorityBits) & (uint32_t)((1UL << (PreemptPriorityBits)) - 1UL);
1723 *pSubPriority = (Priority ) & (uint32_t)((1UL << (SubPriorityBits )) - 1UL);
1724 }
1725
1726
1736 __STATIC_INLINE void __NVIC_SetVector(IRQn_Type IRQn, uint32_t vector)
1737 {
1738 uint32_t *vectors = (uint32_t *)SCB->VTOR;
1739 vectors[(int32_t)IRQn + NVIC_USER_IRQ_OFFSET] = vector;
1740 }
1741
1742
1751 __STATIC_INLINE uint32_t __NVIC_GetVector(IRQn_Type IRQn)
1752 {
1753 uint32_t *vectors = (uint32_t *)SCB->VTOR;
1754 return vectors[(int32_t)IRQn + NVIC_USER_IRQ_OFFSET];
1755 }
1756
1757
1762 __NO_RETURN __STATIC_INLINE void __NVIC_SystemReset(void)
1763 {
1764 __DSB(); /* Ensure all outstanding memory accesses included
1765 buffered write are completed before reset */
1766 SCB->AIRCR = (uint32_t)((0x5FAUL << SCB_AIRCR_VECTKEY_Pos) |
1767 (SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) |
1768 SCB_AIRCR_SYSRESETREQ_Msk ); /* Keep priority group unchanged */
1769 __DSB(); /* Ensure completion of memory access */
1770
1771 for(;;) /* wait until reset */
1772 {
1773 __NOP();
1774 }
1775 }
1776
1779 /* ########################## MPU functions #################################### */
1780
1781 #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1782
1783 #include "mpu_armv7.h"
1784
1785 #endif
1786
1787 /* ########################## FPU functions #################################### */
1803 __STATIC_INLINE uint32_t SCB_GetFPUType(void)
1804 {
1805 return 0U; /* No FPU */
1806 }
1807
1808
1813 /* ################################## SysTick function ############################################ */
1821 #if defined (__Vendor_SysTickConfig) && (__Vendor_SysTickConfig == 0U)
1822
1834 __STATIC_INLINE uint32_t SysTick_Config(uint32_t ticks)
1835 {
1836 if ((ticks - 1UL) > SysTick_LOAD_RELOAD_Msk)
1837 {
1838 return (1UL); /* Reload value impossible */
1839 }
1840
1841 SysTick->LOAD = (uint32_t)(ticks - 1UL); /* set reload register */
1842 NVIC_SetPriority (SysTick_IRQn, (1UL << __NVIC_PRIO_BITS) - 1UL); /* set Priority for Systick Interrupt */
1843 SysTick->VAL = 0UL; /* Load the SysTick Counter Value */
1844 SysTick->CTRL = SysTick_CTRL_CLKSOURCE_Msk |
1845 SysTick_CTRL_TICKINT_Msk |
1846 SysTick_CTRL_ENABLE_Msk; /* Enable SysTick IRQ and SysTick Timer */
1847 return (0UL); /* Function successful */
1848 }
1849
1850 #endif
1851
1856 /* ##################################### Debug In/Output function ########################################### */
1864 extern volatile int32_t ITM_RxBuffer;
1865 #define ITM_RXBUFFER_EMPTY ((int32_t)0x5AA55AA5U)
1876 __STATIC_INLINE uint32_t ITM_SendChar (uint32_t ch)
1877 {
1878 if (((ITM->TCR & ITM_TCR_ITMENA_Msk) != 0UL) && /* ITM enabled */
1879 ((ITM->TER & 1UL ) != 0UL) ) /* ITM Port #0 enabled */
1880 {
1881 while (ITM->PORT[0U].u32 == 0UL)
1882 {
1883 __NOP();
1884 }
1885 ITM->PORT[0U].u8 = (uint8_t)ch;
1886 }
1887 return (ch);
1888 }
1889
1890
1897 __STATIC_INLINE int32_t ITM_ReceiveChar (void)
1898 {
1899 int32_t ch = -1; /* no character available */
1900
1901 if (ITM_RxBuffer != ITM_RXBUFFER_EMPTY)
1902 {
1903 ch = ITM_RxBuffer;
1904 ITM_RxBuffer = ITM_RXBUFFER_EMPTY; /* ready for next character */
1905 }
1906
1907 return (ch);
1908 }
1909
1910
1917 __STATIC_INLINE int32_t ITM_CheckChar (void)
1918 {
1919
1920 if (ITM_RxBuffer == ITM_RXBUFFER_EMPTY)
1921 {
1922 return (0); /* no character available */
1923 }
1924 else
1925 {
1926 return (1); /* character available */
1927 }
1928 }
1929
1935 #ifdef __cplusplus
1936 }
1937 #endif
1938
1939 #endif /* __CORE_CM3_H_DEPENDANT */
1940
1941 #endif /* __CMSIS_GENERIC */
ITM
#define ITM
Definition: core_cm3.h:1396
DWT_Type
Structure type to access the Data Watchpoint and Trace Register (DWT).
Definition: core_cm3.h:849
__NOP
#define __NOP
No Operation
Definition: cmsis_armcc.h:387
SCB_AIRCR_PRIGROUP_Msk
#define SCB_AIRCR_PRIGROUP_Msk
Definition: core_cm3.h:469
CONTROL_Type::nPRIV
uint32_t nPRIV
Definition: core_cm3.h:313
CONTROL_Type::SPSEL
uint32_t SPSEL
Definition: core_cm3.h:314
CONTROL_Type::_reserved1
uint32_t _reserved1
Definition: core_cm3.h:315
__NVIC_GetEnableIRQ
__STATIC_INLINE uint32_t __NVIC_GetEnableIRQ(IRQn_Type IRQn)
Get Interrupt Enable status
Definition: core_cm3.h:1528
SCB_AIRCR_VECTKEY_Msk
#define SCB_AIRCR_VECTKEY_Msk
Definition: core_cm3.h:460
SysTick
#define SysTick
Definition: core_cm3.h:1394
ITM_RXBUFFER_EMPTY
#define ITM_RXBUFFER_EMPTY
Definition: core_cm3.h:1865
APSR_Type::Z
uint32_t Z
Definition: core_cm3.h:214
IPSR_Type::w
uint32_t w
Definition: core_cm3.h:247
__NVIC_GetVector
__STATIC_INLINE uint32_t __NVIC_GetVector(IRQn_Type IRQn)
Get Interrupt Vector
Definition: core_cm3.h:1751
xPSR_Type::_reserved1
uint32_t _reserved1
Definition: core_cm3.h:265
__NVIC_EnableIRQ
__STATIC_INLINE void __NVIC_EnableIRQ(IRQn_Type IRQn)
Enable Interrupt
Definition: core_cm3.h:1511
__NVIC_GetPendingIRQ
__STATIC_INLINE uint32_t __NVIC_GetPendingIRQ(IRQn_Type IRQn)
Get Pending Interrupt
Definition: core_cm3.h:1566
ITM_RxBuffer
volatile int32_t ITM_RxBuffer
ITM_ReceiveChar
__STATIC_INLINE int32_t ITM_ReceiveChar(void)
ITM Receive Character
Definition: core_cm3.h:1897
xPSR_Type::ICI_IT_1
uint32_t ICI_IT_1
Definition: core_cm3.h:264
__NVIC_SetPendingIRQ
__STATIC_INLINE void __NVIC_SetPendingIRQ(IRQn_Type IRQn)
Set Pending Interrupt
Definition: core_cm3.h:1585
xPSR_Type::ISR
uint32_t ISR
Definition: core_cm3.h:262
IPSR_Type
Union type to access the Interrupt Program Status Register (IPSR).
Definition: core_cm3.h:240
TPI_Type
Structure type to access the Trace Port Interface Register (TPI).
Definition: core_cm3.h:996
xPSR_Type::w
uint32_t w
Definition: core_cm3.h:274
ITM_CheckChar
__STATIC_INLINE int32_t ITM_CheckChar(void)
ITM Check Character
Definition: core_cm3.h:1917
SCB_GetFPUType
__STATIC_INLINE uint32_t SCB_GetFPUType(void)
get FPU type
Definition: core_cm3.h:1803
NVIC_DecodePriority
__STATIC_INLINE void NVIC_DecodePriority(uint32_t Priority, uint32_t PriorityGroup, uint32_t *const pPreemptPriority, uint32_t *const pSubPriority)
Decode Priority
Definition: core_cm3.h:1713
NVIC
#define NVIC
Definition: core_cm3.h:1395
__DSB
__STATIC_FORCEINLINE void __DSB(void)
Data Synchronization Barrier
Definition: cmsis_gcc.h:877
xPSR_Type::Q
uint32_t Q
Definition: core_cm3.h:268
cmsis_version.h
CMSIS Core(M) Version definitions
CoreDebug_Type
Structure type to access the Core Debug Register (CoreDebug).
Definition: core_cm3.h:1254
SCB_Type
Structure type to access the System Control Block (SCB).
Definition: core_cm3.h:374
ITM_TCR_ITMENA_Msk
#define ITM_TCR_ITMENA_Msk
Definition: core_cm3.h:812
SCB
#define SCB
Definition: core_cm3.h:1393
ITM_Type
Structure type to access the Instrumentation Trace Macrocell Register (ITM).
Definition: core_cm3.h:746
APSR_Type::N
uint32_t N
Definition: core_cm3.h:215
xPSR_Type::C
uint32_t C
Definition: core_cm3.h:270
__NVIC_SetVector
__STATIC_INLINE void __NVIC_SetVector(IRQn_Type IRQn, uint32_t vector)
Set Interrupt Vector
Definition: core_cm3.h:1736
__NVIC_GetPriorityGrouping
__STATIC_INLINE uint32_t __NVIC_GetPriorityGrouping(void)
Get Priority Grouping
Definition: core_cm3.h:1499
__NVIC_DisableIRQ
__STATIC_INLINE void __NVIC_DisableIRQ(IRQn_Type IRQn)
Disable Interrupt
Definition: core_cm3.h:1547
APSR_Type::_reserved0
uint32_t _reserved0
Definition: core_cm3.h:210
SCB_AIRCR_PRIGROUP_Pos
#define SCB_AIRCR_PRIGROUP_Pos
Definition: core_cm3.h:468
SCnSCB_Type
Structure type to access the System Control and ID Register not in the SCB.
Definition: core_cm3.h:655
xPSR_Type::_reserved0
uint32_t _reserved0
Definition: core_cm3.h:263
NVIC_Type
Structure type to access the Nested Vectored Interrupt Controller (NVIC).
Definition: core_cm3.h:340
SysTick_Type
Structure type to access the System Timer (SysTick).
Definition: core_cm3.h:694
SCB_AIRCR_VECTKEY_Pos
#define SCB_AIRCR_VECTKEY_Pos
Definition: core_cm3.h:459
xPSR_Type::T
uint32_t T
Definition: core_cm3.h:266
APSR_Type::w
uint32_t w
Definition: core_cm3.h:217
APSR_Type::Q
uint32_t Q
Definition: core_cm3.h:211
__NVIC_GetActive
__STATIC_INLINE uint32_t __NVIC_GetActive(IRQn_Type IRQn)
Get Active Interrupt
Definition: core_cm3.h:1617
__NVIC_SetPriority
__STATIC_INLINE void __NVIC_SetPriority(IRQn_Type IRQn, uint32_t priority)
Set Interrupt Priority
Definition: core_cm3.h:1639
APSR_Type::C
uint32_t C
Definition: core_cm3.h:213
xPSR_Type::N
uint32_t N
Definition: core_cm3.h:272
SCB_AIRCR_SYSRESETREQ_Msk
#define SCB_AIRCR_SYSRESETREQ_Msk
Definition: core_cm3.h:472
cmsis_compiler.h
CMSIS compiler generic header file
APSR_Type
Union type to access the Application Program Status Register (APSR).
Definition: core_cm3.h:206
SysTick_LOAD_RELOAD_Msk
#define SysTick_LOAD_RELOAD_Msk
Definition: core_cm3.h:717
IPSR_Type::ISR
uint32_t ISR
Definition: core_cm3.h:244
__NVIC_ClearPendingIRQ
__STATIC_INLINE void __NVIC_ClearPendingIRQ(IRQn_Type IRQn)
Clear Pending Interrupt
Definition: core_cm3.h:1600
CONTROL_Type
Union type to access the Control Registers (CONTROL).
Definition: core_cm3.h:309
SysTick_CTRL_CLKSOURCE_Msk
#define SysTick_CTRL_CLKSOURCE_Msk
Definition: core_cm3.h:707
xPSR_Type::ICI_IT_2
uint32_t ICI_IT_2
Definition: core_cm3.h:267
SysTick_CTRL_ENABLE_Msk
#define SysTick_CTRL_ENABLE_Msk
Definition: core_cm3.h:713
xPSR_Type::V
uint32_t V
Definition: core_cm3.h:269
APSR_Type::V
uint32_t V
Definition: core_cm3.h:212
CONTROL_Type::w
uint32_t w
Definition: core_cm3.h:317
NVIC_EncodePriority
__STATIC_INLINE uint32_t NVIC_EncodePriority(uint32_t PriorityGroup, uint32_t PreemptPriority, uint32_t SubPriority)
Encode Priority
Definition: core_cm3.h:1686
__NVIC_SystemReset
__NO_RETURN __STATIC_INLINE void __NVIC_SystemReset(void)
System Reset
Definition: core_cm3.h:1762
xPSR_Type
Union type to access the Special-Purpose Program Status Registers (xPSR).
Definition: core_cm3.h:258
xPSR_Type::Z
uint32_t Z
Definition: core_cm3.h:271
__ISB
__STATIC_FORCEINLINE void __ISB(void)
Instruction Synchronization Barrier
Definition: cmsis_gcc.h:866
__NVIC_GetPriority
__STATIC_INLINE uint32_t __NVIC_GetPriority(IRQn_Type IRQn)
Get Interrupt Priority
Definition: core_cm3.h:1661
IPSR_Type::_reserved0
uint32_t _reserved0
Definition: core_cm3.h:245
SysTick_CTRL_TICKINT_Msk
#define SysTick_CTRL_TICKINT_Msk
Definition: core_cm3.h:710
__NVIC_SetPriorityGrouping
__STATIC_INLINE void __NVIC_SetPriorityGrouping(uint32_t PriorityGroup)
Set Priority Grouping
Definition: core_cm3.h:1480