MG32F10x Standard Peripherals Firmware Library

成员变量
I2S_TypeDef结构体 参考
CMSIS » Mg32f10x

## 成员变量
__IOM uint32_t | IER
__IOM uint32_t | IRER
__IOM uint32_t | ITER
__IOM uint32_t | CER
__IOM uint32_t | CCR
__OM uint32_t | RXFFR
__OM uint32_t | TXFFR
uint32_t | RESERVED0
struct {
union {
__IM uint32_t LRBR
__OM uint32_t LTHR
} |
union {
__IM uint32_t RRBR
__OM uint32_t RTHR
} |
__IOM uint32_t RER
__IOM uint32_t TER
__IOM uint32_t RCR
__IOM uint32_t TCR
__IM uint32_t ISR
__IOM uint32_t IMR
__IM uint32_t ROR
__IM uint32_t TOR
__IOM uint32_t RFCR
__IOM uint32_t TFCR
__OM uint32_t RFF
__OM uint32_t TFF
uint32_t RESERVED0
uint32_t RESERVED1
} | Ch [2]
__IM uint32_t | RXDMA
__OM uint32_t | RRXDMA
__OM uint32_t | TXDMA
__OM uint32_t | RTXDMA

## 结构体成员变量说明

## ◆ CCR

__IOM uint32_t CCR

Clock Configuration Register, Address offset: 0x010

## ◆ CER

__IOM uint32_t CER

Clock Enable Register, Address offset: 0x00C

## ◆ IER

__IOM uint32_t IER

I2S Enable Register, Address offset: 0x000

## ◆ IMR

__IOM uint32_t IMR

Interrupt Mask Register, Address offset: 0x03C, 0x07C

## ◆ IRER

__IOM uint32_t IRER

I2S Receiver Block Enable Register, Address offset: 0x004

## ◆ ISR

__IM uint32_t ISR

Interrupt Status Register, Address offset: 0x038, 0x078

## ◆ ITER

__IOM uint32_t ITER

I2S Transmitter Block Enable Register, Address offset: 0x008

## ◆ LRBR

__IM uint32_t LRBR

Left Receive Buffer Register, Address offset: 0x020, 0x060

## ◆ LTHR

__OM uint32_t LTHR

Left Transmit Holding Register, Address offset: 0x020, 0x060

## ◆ RCR

__IOM uint32_t RCR

Receive Configuration Register, Address offset: 0x030, 0x070

## ◆ RER

__IOM uint32_t RER

Receive Enable Register, Address offset: 0x028, 0x068

## ◆ RESERVED0

uint32_t RESERVED0

Reserved, 0x01C

## ◆ RESERVED1

uint32_t RESERVED1

Reserved, 0x0A0 - 0x1BC

## ◆ RFCR

__IOM uint32_t RFCR

Receive FIFO Configuration Register, Address offset: 0x048, 0x088

## ◆ RFF

__OM uint32_t RFF

Receive FIFO Flush Register, Address offset: 0x050, 0x090

## ◆ ROR

__IM uint32_t ROR

Receive Overrun Register, Address offset: 0x040, 0x080

## ◆ RRBR

__IM uint32_t RRBR

Right Receive Buffer Register, Address offset: 0x024, 0x064

## ◆ RRXDMA

__OM uint32_t RRXDMA

Reset Receiver Block DMA Register, Address offset: 0x1C4

## ◆ RTHR

__OM uint32_t RTHR

Right Transmit Holding Register, Address offset: 0x024, 0x064

## ◆ RTXDMA

__OM uint32_t RTXDMA

Reset Transmitter Block DMA Register, Address offset: 0x1CC

## ◆ RXDMA

__IM uint32_t RXDMA

Receiver Block DMA Register, Address offset: 0x1C0

## ◆ RXFFR

__OM uint32_t RXFFR

Receiver Block FIFO Reset Register, Address offset: 0x014

## ◆ TCR

__IOM uint32_t TCR

Transmit Configuration Register, Address offset: 0x034, 0x074

## ◆ TER

__IOM uint32_t TER

Transmit Enable Register, Address offset: 0x02C, 0x06C

## ◆ TFCR

__IOM uint32_t TFCR

Transmit FIFO Configuration Register, Address offset: 0x04C, 0x08C

## ◆ TFF

__OM uint32_t TFF

Transmit FIFO Flush Register, Address offset: 0x054, 0x094

## ◆ TOR

__IM uint32_t TOR

Transmit Overrun Register, Address offset: 0x044, 0x084

## ◆ TXDMA

__OM uint32_t TXDMA

Transmitter Block DMA Register, Address offset: 0x1C8

## ◆ TXFFR

__OM uint32_t TXFFR

Transmitter Block FIFO Reset Register, Address offset: 0x018

该结构体的文档由以下文件生成:

- mg32f10x.h