MG32F10x Standard Peripherals Firmware Library

结构体 | 宏定义
Trace Port Interface (TPI)
Defines and Type Definitions

Type definitions for the Trace Port Interface (TPI) 更多...

## 结构体
struct | TPI_Type
| Structure type to access the Trace Port Interface Register (TPI). 更多...

## 宏定义
#define | TPI_ACPR_PRESCALER_Pos 0U
#define | TPI_ACPR_PRESCALER_Msk (0x1FFFUL /*<< TPI_ACPR_PRESCALER_Pos*/)
#define | TPI_SPPR_TXMODE_Pos 0U
#define | TPI_SPPR_TXMODE_Msk (0x3UL /*<< TPI_SPPR_TXMODE_Pos*/)
#define | TPI_FFSR_FtNonStop_Pos 3U
#define | TPI_FFSR_FtNonStop_Msk (0x1UL << TPI_FFSR_FtNonStop_Pos)
#define | TPI_FFSR_TCPresent_Pos 2U
#define | TPI_FFSR_TCPresent_Msk (0x1UL << TPI_FFSR_TCPresent_Pos)
#define | TPI_FFSR_FtStopped_Pos 1U
#define | TPI_FFSR_FtStopped_Msk (0x1UL << TPI_FFSR_FtStopped_Pos)
#define | TPI_FFSR_FlInProg_Pos 0U
#define | TPI_FFSR_FlInProg_Msk (0x1UL /*<< TPI_FFSR_FlInProg_Pos*/)
#define | TPI_FFCR_TrigIn_Pos 8U
#define | TPI_FFCR_TrigIn_Msk (0x1UL << TPI_FFCR_TrigIn_Pos)
#define | TPI_FFCR_EnFCont_Pos 1U
#define | TPI_FFCR_EnFCont_Msk (0x1UL << TPI_FFCR_EnFCont_Pos)
#define | TPI_TRIGGER_TRIGGER_Pos 0U
#define | TPI_TRIGGER_TRIGGER_Msk (0x1UL /*<< TPI_TRIGGER_TRIGGER_Pos*/)
#define | TPI_FIFO0_ITM_ATVALID_Pos 29U
#define | TPI_FIFO0_ITM_ATVALID_Msk (0x3UL << TPI_FIFO0_ITM_ATVALID_Pos)
#define | TPI_FIFO0_ITM_bytecount_Pos 27U
#define | TPI_FIFO0_ITM_bytecount_Msk (0x3UL << TPI_FIFO0_ITM_bytecount_Pos)
#define | TPI_FIFO0_ETM_ATVALID_Pos 26U
#define | TPI_FIFO0_ETM_ATVALID_Msk (0x3UL << TPI_FIFO0_ETM_ATVALID_Pos)
#define | TPI_FIFO0_ETM_bytecount_Pos 24U
#define | TPI_FIFO0_ETM_bytecount_Msk (0x3UL << TPI_FIFO0_ETM_bytecount_Pos)
#define | TPI_FIFO0_ETM2_Pos 16U
#define | TPI_FIFO0_ETM2_Msk (0xFFUL << TPI_FIFO0_ETM2_Pos)
#define | TPI_FIFO0_ETM1_Pos 8U
#define | TPI_FIFO0_ETM1_Msk (0xFFUL << TPI_FIFO0_ETM1_Pos)
#define | TPI_FIFO0_ETM0_Pos 0U
#define | TPI_FIFO0_ETM0_Msk (0xFFUL /*<< TPI_FIFO0_ETM0_Pos*/)
#define | TPI_ITATBCTR2_ATREADY2_Pos 0U
#define | TPI_ITATBCTR2_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY2_Pos*/)
#define | TPI_ITATBCTR2_ATREADY1_Pos 0U
#define | TPI_ITATBCTR2_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY1_Pos*/)
#define | TPI_FIFO1_ITM_ATVALID_Pos 29U
#define | TPI_FIFO1_ITM_ATVALID_Msk (0x3UL << TPI_FIFO1_ITM_ATVALID_Pos)
#define | TPI_FIFO1_ITM_bytecount_Pos 27U
#define | TPI_FIFO1_ITM_bytecount_Msk (0x3UL << TPI_FIFO1_ITM_bytecount_Pos)
#define | TPI_FIFO1_ETM_ATVALID_Pos 26U
#define | TPI_FIFO1_ETM_ATVALID_Msk (0x3UL << TPI_FIFO1_ETM_ATVALID_Pos)
#define | TPI_FIFO1_ETM_bytecount_Pos 24U
#define | TPI_FIFO1_ETM_bytecount_Msk (0x3UL << TPI_FIFO1_ETM_bytecount_Pos)
#define | TPI_FIFO1_ITM2_Pos 16U
#define | TPI_FIFO1_ITM2_Msk (0xFFUL << TPI_FIFO1_ITM2_Pos)
#define | TPI_FIFO1_ITM1_Pos 8U
#define | TPI_FIFO1_ITM1_Msk (0xFFUL << TPI_FIFO1_ITM1_Pos)
#define | TPI_FIFO1_ITM0_Pos 0U
#define | TPI_FIFO1_ITM0_Msk (0xFFUL /*<< TPI_FIFO1_ITM0_Pos*/)
#define | TPI_ITATBCTR0_ATREADY2_Pos 0U
#define | TPI_ITATBCTR0_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY2_Pos*/)
#define | TPI_ITATBCTR0_ATREADY1_Pos 0U
#define | TPI_ITATBCTR0_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY1_Pos*/)
#define | TPI_ITCTRL_Mode_Pos 0U
#define | TPI_ITCTRL_Mode_Msk (0x3UL /*<< TPI_ITCTRL_Mode_Pos*/)
#define | TPI_DEVID_NRZVALID_Pos 11U
#define | TPI_DEVID_NRZVALID_Msk (0x1UL << TPI_DEVID_NRZVALID_Pos)
#define | TPI_DEVID_MANCVALID_Pos 10U
#define | TPI_DEVID_MANCVALID_Msk (0x1UL << TPI_DEVID_MANCVALID_Pos)
#define | TPI_DEVID_PTINVALID_Pos 9U
#define | TPI_DEVID_PTINVALID_Msk (0x1UL << TPI_DEVID_PTINVALID_Pos)
#define | TPI_DEVID_MinBufSz_Pos 6U
#define | TPI_DEVID_MinBufSz_Msk (0x7UL << TPI_DEVID_MinBufSz_Pos)
#define | TPI_DEVID_AsynClkIn_Pos 5U
#define | TPI_DEVID_AsynClkIn_Msk (0x1UL << TPI_DEVID_AsynClkIn_Pos)
#define | TPI_DEVID_NrTraceInput_Pos 0U
#define | TPI_DEVID_NrTraceInput_Msk (0x1FUL /*<< TPI_DEVID_NrTraceInput_Pos*/)
#define | TPI_DEVTYPE_SubType_Pos 4U
#define | TPI_DEVTYPE_SubType_Msk (0xFUL /*<< TPI_DEVTYPE_SubType_Pos*/)
#define | TPI_DEVTYPE_MajorType_Pos 0U
#define | TPI_DEVTYPE_MajorType_Msk (0xFUL << TPI_DEVTYPE_MajorType_Pos)

## 详细描述

Type definitions for the Trace Port Interface (TPI)

## 宏定义说明

## ◆ TPI_ACPR_PRESCALER_Msk

#define TPI_ACPR_PRESCALER_Msk (0x1FFFUL /*<< TPI_ACPR_PRESCALER_Pos*/)

TPI ACPR: PRESCALER Mask

## ◆ TPI_ACPR_PRESCALER_Pos

#define TPI_ACPR_PRESCALER_Pos 0U

TPI ACPR: PRESCALER Position

## ◆ TPI_DEVID_AsynClkIn_Msk

#define TPI_DEVID_AsynClkIn_Msk (0x1UL << TPI_DEVID_AsynClkIn_Pos)

TPI DEVID: AsynClkIn Mask

## ◆ TPI_DEVID_AsynClkIn_Pos

#define TPI_DEVID_AsynClkIn_Pos 5U

TPI DEVID: AsynClkIn Position

## ◆ TPI_DEVID_MANCVALID_Msk

#define TPI_DEVID_MANCVALID_Msk (0x1UL << TPI_DEVID_MANCVALID_Pos)

TPI DEVID: MANCVALID Mask

## ◆ TPI_DEVID_MANCVALID_Pos

#define TPI_DEVID_MANCVALID_Pos 10U

TPI DEVID: MANCVALID Position

## ◆ TPI_DEVID_MinBufSz_Msk

#define TPI_DEVID_MinBufSz_Msk (0x7UL << TPI_DEVID_MinBufSz_Pos)

TPI DEVID: MinBufSz Mask

## ◆ TPI_DEVID_MinBufSz_Pos

#define TPI_DEVID_MinBufSz_Pos 6U

TPI DEVID: MinBufSz Position

## ◆ TPI_DEVID_NrTraceInput_Msk

#define TPI_DEVID_NrTraceInput_Msk (0x1FUL /*<< TPI_DEVID_NrTraceInput_Pos*/)

TPI DEVID: NrTraceInput Mask

## ◆ TPI_DEVID_NrTraceInput_Pos

#define TPI_DEVID_NrTraceInput_Pos 0U

TPI DEVID: NrTraceInput Position

## ◆ TPI_DEVID_NRZVALID_Msk

#define TPI_DEVID_NRZVALID_Msk (0x1UL << TPI_DEVID_NRZVALID_Pos)

TPI DEVID: NRZVALID Mask

## ◆ TPI_DEVID_NRZVALID_Pos

#define TPI_DEVID_NRZVALID_Pos 11U

TPI DEVID: NRZVALID Position

## ◆ TPI_DEVID_PTINVALID_Msk

#define TPI_DEVID_PTINVALID_Msk (0x1UL << TPI_DEVID_PTINVALID_Pos)

TPI DEVID: PTINVALID Mask

## ◆ TPI_DEVID_PTINVALID_Pos

#define TPI_DEVID_PTINVALID_Pos 9U

TPI DEVID: PTINVALID Position

## ◆ TPI_DEVTYPE_MajorType_Msk

#define TPI_DEVTYPE_MajorType_Msk (0xFUL << TPI_DEVTYPE_MajorType_Pos)

TPI DEVTYPE: MajorType Mask

## ◆ TPI_DEVTYPE_MajorType_Pos

#define TPI_DEVTYPE_MajorType_Pos 0U

TPI DEVTYPE: MajorType Position

## ◆ TPI_DEVTYPE_SubType_Msk

#define TPI_DEVTYPE_SubType_Msk (0xFUL /*<< TPI_DEVTYPE_SubType_Pos*/)

TPI DEVTYPE: SubType Mask

## ◆ TPI_DEVTYPE_SubType_Pos

#define TPI_DEVTYPE_SubType_Pos 4U

TPI DEVTYPE: SubType Position

## ◆ TPI_FFCR_EnFCont_Msk

#define TPI_FFCR_EnFCont_Msk (0x1UL << TPI_FFCR_EnFCont_Pos)

TPI FFCR: EnFCont Mask

## ◆ TPI_FFCR_EnFCont_Pos

#define TPI_FFCR_EnFCont_Pos 1U

TPI FFCR: EnFCont Position

## ◆ TPI_FFCR_TrigIn_Msk

#define TPI_FFCR_TrigIn_Msk (0x1UL << TPI_FFCR_TrigIn_Pos)

TPI FFCR: TrigIn Mask

## ◆ TPI_FFCR_TrigIn_Pos

#define TPI_FFCR_TrigIn_Pos 8U

TPI FFCR: TrigIn Position

## ◆ TPI_FFSR_FlInProg_Msk

#define TPI_FFSR_FlInProg_Msk (0x1UL /*<< TPI_FFSR_FlInProg_Pos*/)

TPI FFSR: FlInProg Mask

## ◆ TPI_FFSR_FlInProg_Pos

#define TPI_FFSR_FlInProg_Pos 0U

TPI FFSR: FlInProg Position

## ◆ TPI_FFSR_FtNonStop_Msk

#define TPI_FFSR_FtNonStop_Msk (0x1UL << TPI_FFSR_FtNonStop_Pos)

TPI FFSR: FtNonStop Mask

## ◆ TPI_FFSR_FtNonStop_Pos

#define TPI_FFSR_FtNonStop_Pos 3U

TPI FFSR: FtNonStop Position

## ◆ TPI_FFSR_FtStopped_Msk

#define TPI_FFSR_FtStopped_Msk (0x1UL << TPI_FFSR_FtStopped_Pos)

TPI FFSR: FtStopped Mask

## ◆ TPI_FFSR_FtStopped_Pos

#define TPI_FFSR_FtStopped_Pos 1U

TPI FFSR: FtStopped Position

## ◆ TPI_FFSR_TCPresent_Msk

#define TPI_FFSR_TCPresent_Msk (0x1UL << TPI_FFSR_TCPresent_Pos)

TPI FFSR: TCPresent Mask

## ◆ TPI_FFSR_TCPresent_Pos

#define TPI_FFSR_TCPresent_Pos 2U

TPI FFSR: TCPresent Position

## ◆ TPI_FIFO0_ETM0_Msk

#define TPI_FIFO0_ETM0_Msk (0xFFUL /*<< TPI_FIFO0_ETM0_Pos*/)

TPI FIFO0: ETM0 Mask

## ◆ TPI_FIFO0_ETM0_Pos

#define TPI_FIFO0_ETM0_Pos 0U

TPI FIFO0: ETM0 Position

## ◆ TPI_FIFO0_ETM1_Msk

#define TPI_FIFO0_ETM1_Msk (0xFFUL << TPI_FIFO0_ETM1_Pos)

TPI FIFO0: ETM1 Mask

## ◆ TPI_FIFO0_ETM1_Pos

#define TPI_FIFO0_ETM1_Pos 8U

TPI FIFO0: ETM1 Position

## ◆ TPI_FIFO0_ETM2_Msk

#define TPI_FIFO0_ETM2_Msk (0xFFUL << TPI_FIFO0_ETM2_Pos)

TPI FIFO0: ETM2 Mask

## ◆ TPI_FIFO0_ETM2_Pos

#define TPI_FIFO0_ETM2_Pos 16U

TPI FIFO0: ETM2 Position

## ◆ TPI_FIFO0_ETM_ATVALID_Msk

#define TPI_FIFO0_ETM_ATVALID_Msk (0x3UL << TPI_FIFO0_ETM_ATVALID_Pos)

TPI FIFO0: ETM_ATVALID Mask

## ◆ TPI_FIFO0_ETM_ATVALID_Pos

#define TPI_FIFO0_ETM_ATVALID_Pos 26U

TPI FIFO0: ETM_ATVALID Position

## ◆ TPI_FIFO0_ETM_bytecount_Msk

#define TPI_FIFO0_ETM_bytecount_Msk (0x3UL << TPI_FIFO0_ETM_bytecount_Pos)

TPI FIFO0: ETM_bytecount Mask

## ◆ TPI_FIFO0_ETM_bytecount_Pos

#define TPI_FIFO0_ETM_bytecount_Pos 24U

TPI FIFO0: ETM_bytecount Position

## ◆ TPI_FIFO0_ITM_ATVALID_Msk

#define TPI_FIFO0_ITM_ATVALID_Msk (0x3UL << TPI_FIFO0_ITM_ATVALID_Pos)

TPI FIFO0: ITM_ATVALID Mask

## ◆ TPI_FIFO0_ITM_ATVALID_Pos

#define TPI_FIFO0_ITM_ATVALID_Pos 29U

TPI FIFO0: ITM_ATVALID Position

## ◆ TPI_FIFO0_ITM_bytecount_Msk

#define TPI_FIFO0_ITM_bytecount_Msk (0x3UL << TPI_FIFO0_ITM_bytecount_Pos)

TPI FIFO0: ITM_bytecount Mask

## ◆ TPI_FIFO0_ITM_bytecount_Pos

#define TPI_FIFO0_ITM_bytecount_Pos 27U

TPI FIFO0: ITM_bytecount Position

## ◆ TPI_FIFO1_ETM_ATVALID_Msk

#define TPI_FIFO1_ETM_ATVALID_Msk (0x3UL << TPI_FIFO1_ETM_ATVALID_Pos)

TPI FIFO1: ETM_ATVALID Mask

## ◆ TPI_FIFO1_ETM_ATVALID_Pos

#define TPI_FIFO1_ETM_ATVALID_Pos 26U

TPI FIFO1: ETM_ATVALID Position

## ◆ TPI_FIFO1_ETM_bytecount_Msk

#define TPI_FIFO1_ETM_bytecount_Msk (0x3UL << TPI_FIFO1_ETM_bytecount_Pos)

TPI FIFO1: ETM_bytecount Mask

## ◆ TPI_FIFO1_ETM_bytecount_Pos

#define TPI_FIFO1_ETM_bytecount_Pos 24U

TPI FIFO1: ETM_bytecount Position

## ◆ TPI_FIFO1_ITM0_Msk

#define TPI_FIFO1_ITM0_Msk (0xFFUL /*<< TPI_FIFO1_ITM0_Pos*/)

TPI FIFO1: ITM0 Mask

## ◆ TPI_FIFO1_ITM0_Pos

#define TPI_FIFO1_ITM0_Pos 0U

TPI FIFO1: ITM0 Position

## ◆ TPI_FIFO1_ITM1_Msk

#define TPI_FIFO1_ITM1_Msk (0xFFUL << TPI_FIFO1_ITM1_Pos)

TPI FIFO1: ITM1 Mask

## ◆ TPI_FIFO1_ITM1_Pos

#define TPI_FIFO1_ITM1_Pos 8U

TPI FIFO1: ITM1 Position

## ◆ TPI_FIFO1_ITM2_Msk

#define TPI_FIFO1_ITM2_Msk (0xFFUL << TPI_FIFO1_ITM2_Pos)

TPI FIFO1: ITM2 Mask

## ◆ TPI_FIFO1_ITM2_Pos

#define TPI_FIFO1_ITM2_Pos 16U

TPI FIFO1: ITM2 Position

## ◆ TPI_FIFO1_ITM_ATVALID_Msk

#define TPI_FIFO1_ITM_ATVALID_Msk (0x3UL << TPI_FIFO1_ITM_ATVALID_Pos)

TPI FIFO1: ITM_ATVALID Mask

## ◆ TPI_FIFO1_ITM_ATVALID_Pos

#define TPI_FIFO1_ITM_ATVALID_Pos 29U

TPI FIFO1: ITM_ATVALID Position

## ◆ TPI_FIFO1_ITM_bytecount_Msk

#define TPI_FIFO1_ITM_bytecount_Msk (0x3UL << TPI_FIFO1_ITM_bytecount_Pos)

TPI FIFO1: ITM_bytecount Mask

## ◆ TPI_FIFO1_ITM_bytecount_Pos

#define TPI_FIFO1_ITM_bytecount_Pos 27U

TPI FIFO1: ITM_bytecount Position

## ◆ TPI_ITATBCTR0_ATREADY1_Msk

#define TPI_ITATBCTR0_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY1_Pos*/)

TPI ITATBCTR0: ATREADY1 Mask

## ◆ TPI_ITATBCTR0_ATREADY1_Pos

#define TPI_ITATBCTR0_ATREADY1_Pos 0U

TPI ITATBCTR0: ATREADY1 Position

## ◆ TPI_ITATBCTR0_ATREADY2_Msk

#define TPI_ITATBCTR0_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR0_ATREADY2_Pos*/)

TPI ITATBCTR0: ATREADY2 Mask

## ◆ TPI_ITATBCTR0_ATREADY2_Pos

#define TPI_ITATBCTR0_ATREADY2_Pos 0U

TPI ITATBCTR0: ATREADY2 Position

## ◆ TPI_ITATBCTR2_ATREADY1_Msk

#define TPI_ITATBCTR2_ATREADY1_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY1_Pos*/)

TPI ITATBCTR2: ATREADY1 Mask

## ◆ TPI_ITATBCTR2_ATREADY1_Pos

#define TPI_ITATBCTR2_ATREADY1_Pos 0U

TPI ITATBCTR2: ATREADY1 Position

## ◆ TPI_ITATBCTR2_ATREADY2_Msk

#define TPI_ITATBCTR2_ATREADY2_Msk (0x1UL /*<< TPI_ITATBCTR2_ATREADY2_Pos*/)

TPI ITATBCTR2: ATREADY2 Mask

## ◆ TPI_ITATBCTR2_ATREADY2_Pos

#define TPI_ITATBCTR2_ATREADY2_Pos 0U

TPI ITATBCTR2: ATREADY2 Position

## ◆ TPI_ITCTRL_Mode_Msk

#define TPI_ITCTRL_Mode_Msk (0x3UL /*<< TPI_ITCTRL_Mode_Pos*/)

TPI ITCTRL: Mode Mask

## ◆ TPI_ITCTRL_Mode_Pos

#define TPI_ITCTRL_Mode_Pos 0U

TPI ITCTRL: Mode Position

## ◆ TPI_SPPR_TXMODE_Msk

#define TPI_SPPR_TXMODE_Msk (0x3UL /*<< TPI_SPPR_TXMODE_Pos*/)

TPI SPPR: TXMODE Mask

## ◆ TPI_SPPR_TXMODE_Pos

#define TPI_SPPR_TXMODE_Pos 0U

TPI SPPR: TXMODE Position

## ◆ TPI_TRIGGER_TRIGGER_Msk

#define TPI_TRIGGER_TRIGGER_Msk (0x1UL /*<< TPI_TRIGGER_TRIGGER_Pos*/)

TPI TRIGGER: TRIGGER Mask

## ◆ TPI_TRIGGER_TRIGGER_Pos

#define TPI_TRIGGER_TRIGGER_Pos 0U

TPI TRIGGER: TRIGGER Position