MG32F10x Standard Peripherals Firmware Library

成员变量
ANCTL_TypeDef结构体 参考
CMSIS » Mg32f10x

## 成员变量
uint32_t | RESERVED0 [7]
__IOM uint32_t | BGCR2
uint32_t | RESERVED1 [3]
__IOM uint32_t | MHSIENR
__IOM uint32_t | MHSISR
uint32_t | RESERVED2
__IOM uint32_t | FHSIENR
__IOM uint32_t | FHSISR
uint32_t | RESERVED3
__IOM uint32_t | LSIENR
__IOM uint32_t | LSISR
__IOM uint32_t | HSECR0
__IOM uint32_t | HSECR1
uint32_t | RESERVED4
__IOM uint32_t | HSESR
uint32_t | RESERVED5 [6]
__IOM uint32_t | PLLCR
__IOM uint32_t | PLLENR
__IOM uint32_t | PLLSR
__IOM uint32_t | PVDCR
__IOM uint32_t | PVDENR
uint32_t | RESERVED6
__IOM uint32_t | SARENR
__IOM uint32_t | USBPCR
__IOM uint32_t | PORCR
__IOM uint32_t | CMPACR
__IOM uint32_t | CMPBCR
__IOM uint32_t | ISR
__IOM uint32_t | IER
__IOM uint32_t | ICR
__IOM uint32_t | CMPASR
__IOM uint32_t | CMPBSR
__IOM uint32_t | DCSSENR
__IOM uint32_t | DCSSCR

## 结构体成员变量说明

## ◆ BGCR2

__IOM uint32_t BGCR2

BandGap control register 2, Address offset: 0x01C

## ◆ CMPACR

__IOM uint32_t CMPACR

CMPA control register, Address offset: 0x098

## ◆ CMPASR

__IOM uint32_t CMPASR

CMPA status register, Address offset: 0x0AC

## ◆ CMPBCR

__IOM uint32_t CMPBCR

CMPB control register, Address offset: 0x09C

## ◆ CMPBSR

__IOM uint32_t CMPBSR

CMPB status register, Address offset: 0x0B0

## ◆ DCSSCR

__IOM uint32_t DCSSCR

DCSS control register, Address offset: 0x0B8

## ◆ DCSSENR

__IOM uint32_t DCSSENR

DCSS enable register, Address offset: 0x0B4

## ◆ FHSIENR

__IOM uint32_t FHSIENR

FHSI enable register, Address offset: 0x038

## ◆ FHSISR

__IOM uint32_t FHSISR

FHSI status register, Address offset: 0x03C

## ◆ HSECR0

__IOM uint32_t HSECR0

HSE control register 0, Address offset: 0x04C

## ◆ HSECR1

__IOM uint32_t HSECR1

HSE control register 1, Address offset: 0x050

## ◆ HSESR

__IOM uint32_t HSESR

HSE status register, Address offset: 0x058

## ◆ ICR

__IOM uint32_t ICR

Interrupt clear register, Address offset: 0x0A8

## ◆ IER

__IOM uint32_t IER

Interrupt enable register, Address offset: 0x0A4

## ◆ ISR

__IOM uint32_t ISR

Interrupt status register, Address offset: 0x0A0

## ◆ LSIENR

__IOM uint32_t LSIENR

LSI enable register, Address offset: 0x044

## ◆ LSISR

__IOM uint32_t LSISR

LSI status register, Address offset: 0x048

## ◆ MHSIENR

__IOM uint32_t MHSIENR

MHSI enable register, Address offset: 0x02C

## ◆ MHSISR

__IOM uint32_t MHSISR

MHSI status register, Address offset: 0x030

## ◆ PLLCR

__IOM uint32_t PLLCR

PLL control register, Address offset: 0x074

## ◆ PLLENR

__IOM uint32_t PLLENR

PLl enable register, Address offset: 0x078

## ◆ PLLSR

__IOM uint32_t PLLSR

PLL status register, Address offset: 0x07C

## ◆ PORCR

__IOM uint32_t PORCR

POR control register, Address offset: 0x094

## ◆ PVDCR

__IOM uint32_t PVDCR

PVD control register, Address offset: 0x080

## ◆ PVDENR

__IOM uint32_t PVDENR

PVD enable register, Address offset: 0x084

## ◆ RESERVED0

uint32_t RESERVED0[7]

Reserved, 0x000 - 0x018

## ◆ RESERVED1

uint32_t RESERVED1[3]

Reserved, 0x020 - 0x028

## ◆ RESERVED2

uint32_t RESERVED2

Reserved, 0x034

## ◆ RESERVED3

uint32_t RESERVED3

Reserved, 0x040

## ◆ RESERVED4

uint32_t RESERVED4

Reserved, 0x054

## ◆ RESERVED5

uint32_t RESERVED5[6]

Reserved, 0x05C - 0x070

## ◆ RESERVED6

uint32_t RESERVED6

Reserved, 0x088

## ◆ SARENR

__IOM uint32_t SARENR

SAR ADC enable register, Address offset: 0x08C

## ◆ USBPCR

__IOM uint32_t USBPCR

USB PHY control register, Address offset: 0x090

该结构体的文档由以下文件生成:

- mg32f10x.h