MG32F10x Standard Peripherals Firmware Library

结构体 | 宏定义
System Control Block (SCB)
Defines and Type Definitions

Type definitions for the System Control Block Registers 更多...

## 结构体
struct | SCB_Type
| Structure type to access the System Control Block (SCB). 更多...

## 宏定义
#define | SCB_CPUID_IMPLEMENTER_Pos 24U
#define | SCB_CPUID_IMPLEMENTER_Msk (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)
#define | SCB_CPUID_VARIANT_Pos 20U
#define | SCB_CPUID_VARIANT_Msk (0xFUL << SCB_CPUID_VARIANT_Pos)
#define | SCB_CPUID_ARCHITECTURE_Pos 16U
#define | SCB_CPUID_ARCHITECTURE_Msk (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)
#define | SCB_CPUID_PARTNO_Pos 4U
#define | SCB_CPUID_PARTNO_Msk (0xFFFUL << SCB_CPUID_PARTNO_Pos)
#define | SCB_CPUID_REVISION_Pos 0U
#define | SCB_CPUID_REVISION_Msk (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)
#define | SCB_ICSR_NMIPENDSET_Pos 31U
#define | SCB_ICSR_NMIPENDSET_Msk (1UL << SCB_ICSR_NMIPENDSET_Pos)
#define | SCB_ICSR_PENDSVSET_Pos 28U
#define | SCB_ICSR_PENDSVSET_Msk (1UL << SCB_ICSR_PENDSVSET_Pos)
#define | SCB_ICSR_PENDSVCLR_Pos 27U
#define | SCB_ICSR_PENDSVCLR_Msk (1UL << SCB_ICSR_PENDSVCLR_Pos)
#define | SCB_ICSR_PENDSTSET_Pos 26U
#define | SCB_ICSR_PENDSTSET_Msk (1UL << SCB_ICSR_PENDSTSET_Pos)
#define | SCB_ICSR_PENDSTCLR_Pos 25U
#define | SCB_ICSR_PENDSTCLR_Msk (1UL << SCB_ICSR_PENDSTCLR_Pos)
#define | SCB_ICSR_ISRPREEMPT_Pos 23U
#define | SCB_ICSR_ISRPREEMPT_Msk (1UL << SCB_ICSR_ISRPREEMPT_Pos)
#define | SCB_ICSR_ISRPENDING_Pos 22U
#define | SCB_ICSR_ISRPENDING_Msk (1UL << SCB_ICSR_ISRPENDING_Pos)
#define | SCB_ICSR_VECTPENDING_Pos 12U
#define | SCB_ICSR_VECTPENDING_Msk (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)
#define | SCB_ICSR_RETTOBASE_Pos 11U
#define | SCB_ICSR_RETTOBASE_Msk (1UL << SCB_ICSR_RETTOBASE_Pos)
#define | SCB_ICSR_VECTACTIVE_Pos 0U
#define | SCB_ICSR_VECTACTIVE_Msk (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)
#define | SCB_VTOR_TBLOFF_Pos 7U
#define | SCB_VTOR_TBLOFF_Msk (0x1FFFFFFUL << SCB_VTOR_TBLOFF_Pos)
#define | SCB_AIRCR_VECTKEY_Pos 16U
#define | SCB_AIRCR_VECTKEY_Msk (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)
#define | SCB_AIRCR_VECTKEYSTAT_Pos 16U
#define | SCB_AIRCR_VECTKEYSTAT_Msk (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)
#define | SCB_AIRCR_ENDIANESS_Pos 15U
#define | SCB_AIRCR_ENDIANESS_Msk (1UL << SCB_AIRCR_ENDIANESS_Pos)
#define | SCB_AIRCR_PRIGROUP_Pos 8U
#define | SCB_AIRCR_PRIGROUP_Msk (7UL << SCB_AIRCR_PRIGROUP_Pos)
#define | SCB_AIRCR_SYSRESETREQ_Pos 2U
#define | SCB_AIRCR_SYSRESETREQ_Msk (1UL << SCB_AIRCR_SYSRESETREQ_Pos)
#define | SCB_AIRCR_VECTCLRACTIVE_Pos 1U
#define | SCB_AIRCR_VECTCLRACTIVE_Msk (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)
#define | SCB_AIRCR_VECTRESET_Pos 0U
#define | SCB_AIRCR_VECTRESET_Msk (1UL /*<< SCB_AIRCR_VECTRESET_Pos*/)
#define | SCB_SCR_SEVONPEND_Pos 4U
#define | SCB_SCR_SEVONPEND_Msk (1UL << SCB_SCR_SEVONPEND_Pos)
#define | SCB_SCR_SLEEPDEEP_Pos 2U
#define | SCB_SCR_SLEEPDEEP_Msk (1UL << SCB_SCR_SLEEPDEEP_Pos)
#define | SCB_SCR_SLEEPONEXIT_Pos 1U
#define | SCB_SCR_SLEEPONEXIT_Msk (1UL << SCB_SCR_SLEEPONEXIT_Pos)
#define | SCB_CCR_STKALIGN_Pos 9U
#define | SCB_CCR_STKALIGN_Msk (1UL << SCB_CCR_STKALIGN_Pos)
#define | SCB_CCR_BFHFNMIGN_Pos 8U
#define | SCB_CCR_BFHFNMIGN_Msk (1UL << SCB_CCR_BFHFNMIGN_Pos)
#define | SCB_CCR_DIV_0_TRP_Pos 4U
#define | SCB_CCR_DIV_0_TRP_Msk (1UL << SCB_CCR_DIV_0_TRP_Pos)
#define | SCB_CCR_UNALIGN_TRP_Pos 3U
#define | SCB_CCR_UNALIGN_TRP_Msk (1UL << SCB_CCR_UNALIGN_TRP_Pos)
#define | SCB_CCR_USERSETMPEND_Pos 1U
#define | SCB_CCR_USERSETMPEND_Msk (1UL << SCB_CCR_USERSETMPEND_Pos)
#define | SCB_CCR_NONBASETHRDENA_Pos 0U
#define | SCB_CCR_NONBASETHRDENA_Msk (1UL /*<< SCB_CCR_NONBASETHRDENA_Pos*/)
#define | SCB_SHCSR_USGFAULTENA_Pos 18U
#define | SCB_SHCSR_USGFAULTENA_Msk (1UL << SCB_SHCSR_USGFAULTENA_Pos)
#define | SCB_SHCSR_BUSFAULTENA_Pos 17U
#define | SCB_SHCSR_BUSFAULTENA_Msk (1UL << SCB_SHCSR_BUSFAULTENA_Pos)
#define | SCB_SHCSR_MEMFAULTENA_Pos 16U
#define | SCB_SHCSR_MEMFAULTENA_Msk (1UL << SCB_SHCSR_MEMFAULTENA_Pos)
#define | SCB_SHCSR_SVCALLPENDED_Pos 15U
#define | SCB_SHCSR_SVCALLPENDED_Msk (1UL << SCB_SHCSR_SVCALLPENDED_Pos)
#define | SCB_SHCSR_BUSFAULTPENDED_Pos 14U
#define | SCB_SHCSR_BUSFAULTPENDED_Msk (1UL << SCB_SHCSR_BUSFAULTPENDED_Pos)
#define | SCB_SHCSR_MEMFAULTPENDED_Pos 13U
#define | SCB_SHCSR_MEMFAULTPENDED_Msk (1UL << SCB_SHCSR_MEMFAULTPENDED_Pos)
#define | SCB_SHCSR_USGFAULTPENDED_Pos 12U
#define | SCB_SHCSR_USGFAULTPENDED_Msk (1UL << SCB_SHCSR_USGFAULTPENDED_Pos)
#define | SCB_SHCSR_SYSTICKACT_Pos 11U
#define | SCB_SHCSR_SYSTICKACT_Msk (1UL << SCB_SHCSR_SYSTICKACT_Pos)
#define | SCB_SHCSR_PENDSVACT_Pos 10U
#define | SCB_SHCSR_PENDSVACT_Msk (1UL << SCB_SHCSR_PENDSVACT_Pos)
#define | SCB_SHCSR_MONITORACT_Pos 8U
#define | SCB_SHCSR_MONITORACT_Msk (1UL << SCB_SHCSR_MONITORACT_Pos)
#define | SCB_SHCSR_SVCALLACT_Pos 7U
#define | SCB_SHCSR_SVCALLACT_Msk (1UL << SCB_SHCSR_SVCALLACT_Pos)
#define | SCB_SHCSR_USGFAULTACT_Pos 3U
#define | SCB_SHCSR_USGFAULTACT_Msk (1UL << SCB_SHCSR_USGFAULTACT_Pos)
#define | SCB_SHCSR_BUSFAULTACT_Pos 1U
#define | SCB_SHCSR_BUSFAULTACT_Msk (1UL << SCB_SHCSR_BUSFAULTACT_Pos)
#define | SCB_SHCSR_MEMFAULTACT_Pos 0U
#define | SCB_SHCSR_MEMFAULTACT_Msk (1UL /*<< SCB_SHCSR_MEMFAULTACT_Pos*/)
#define | SCB_CFSR_USGFAULTSR_Pos 16U
#define | SCB_CFSR_USGFAULTSR_Msk (0xFFFFUL << SCB_CFSR_USGFAULTSR_Pos)
#define | SCB_CFSR_BUSFAULTSR_Pos 8U
#define | SCB_CFSR_BUSFAULTSR_Msk (0xFFUL << SCB_CFSR_BUSFAULTSR_Pos)
#define | SCB_CFSR_MEMFAULTSR_Pos 0U
#define | SCB_CFSR_MEMFAULTSR_Msk (0xFFUL /*<< SCB_CFSR_MEMFAULTSR_Pos*/)
#define | SCB_CFSR_MMARVALID_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 7U)
#define | SCB_CFSR_MMARVALID_Msk (1UL << SCB_CFSR_MMARVALID_Pos)
#define | SCB_CFSR_MSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 4U)
#define | SCB_CFSR_MSTKERR_Msk (1UL << SCB_CFSR_MSTKERR_Pos)
#define | SCB_CFSR_MUNSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 3U)
#define | SCB_CFSR_MUNSTKERR_Msk (1UL << SCB_CFSR_MUNSTKERR_Pos)
#define | SCB_CFSR_DACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 1U)
#define | SCB_CFSR_DACCVIOL_Msk (1UL << SCB_CFSR_DACCVIOL_Pos)
#define | SCB_CFSR_IACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 0U)
#define | SCB_CFSR_IACCVIOL_Msk (1UL /*<< SCB_CFSR_IACCVIOL_Pos*/)
#define | SCB_CFSR_BFARVALID_Pos (SCB_CFSR_BUSFAULTSR_Pos + 7U)
#define | SCB_CFSR_BFARVALID_Msk (1UL << SCB_CFSR_BFARVALID_Pos)
#define | SCB_CFSR_STKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 4U)
#define | SCB_CFSR_STKERR_Msk (1UL << SCB_CFSR_STKERR_Pos)
#define | SCB_CFSR_UNSTKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 3U)
#define | SCB_CFSR_UNSTKERR_Msk (1UL << SCB_CFSR_UNSTKERR_Pos)
#define | SCB_CFSR_IMPRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 2U)
#define | SCB_CFSR_IMPRECISERR_Msk (1UL << SCB_CFSR_IMPRECISERR_Pos)
#define | SCB_CFSR_PRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 1U)
#define | SCB_CFSR_PRECISERR_Msk (1UL << SCB_CFSR_PRECISERR_Pos)
#define | SCB_CFSR_IBUSERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 0U)
#define | SCB_CFSR_IBUSERR_Msk (1UL << SCB_CFSR_IBUSERR_Pos)
#define | SCB_CFSR_DIVBYZERO_Pos (SCB_CFSR_USGFAULTSR_Pos + 9U)
#define | SCB_CFSR_DIVBYZERO_Msk (1UL << SCB_CFSR_DIVBYZERO_Pos)
#define | SCB_CFSR_UNALIGNED_Pos (SCB_CFSR_USGFAULTSR_Pos + 8U)
#define | SCB_CFSR_UNALIGNED_Msk (1UL << SCB_CFSR_UNALIGNED_Pos)
#define | SCB_CFSR_NOCP_Pos (SCB_CFSR_USGFAULTSR_Pos + 3U)
#define | SCB_CFSR_NOCP_Msk (1UL << SCB_CFSR_NOCP_Pos)
#define | SCB_CFSR_INVPC_Pos (SCB_CFSR_USGFAULTSR_Pos + 2U)
#define | SCB_CFSR_INVPC_Msk (1UL << SCB_CFSR_INVPC_Pos)
#define | SCB_CFSR_INVSTATE_Pos (SCB_CFSR_USGFAULTSR_Pos + 1U)
#define | SCB_CFSR_INVSTATE_Msk (1UL << SCB_CFSR_INVSTATE_Pos)
#define | SCB_CFSR_UNDEFINSTR_Pos (SCB_CFSR_USGFAULTSR_Pos + 0U)
#define | SCB_CFSR_UNDEFINSTR_Msk (1UL << SCB_CFSR_UNDEFINSTR_Pos)
#define | SCB_HFSR_DEBUGEVT_Pos 31U
#define | SCB_HFSR_DEBUGEVT_Msk (1UL << SCB_HFSR_DEBUGEVT_Pos)
#define | SCB_HFSR_FORCED_Pos 30U
#define | SCB_HFSR_FORCED_Msk (1UL << SCB_HFSR_FORCED_Pos)
#define | SCB_HFSR_VECTTBL_Pos 1U
#define | SCB_HFSR_VECTTBL_Msk (1UL << SCB_HFSR_VECTTBL_Pos)
#define | SCB_DFSR_EXTERNAL_Pos 4U
#define | SCB_DFSR_EXTERNAL_Msk (1UL << SCB_DFSR_EXTERNAL_Pos)
#define | SCB_DFSR_VCATCH_Pos 3U
#define | SCB_DFSR_VCATCH_Msk (1UL << SCB_DFSR_VCATCH_Pos)
#define | SCB_DFSR_DWTTRAP_Pos 2U
#define | SCB_DFSR_DWTTRAP_Msk (1UL << SCB_DFSR_DWTTRAP_Pos)
#define | SCB_DFSR_BKPT_Pos 1U
#define | SCB_DFSR_BKPT_Msk (1UL << SCB_DFSR_BKPT_Pos)
#define | SCB_DFSR_HALTED_Pos 0U
#define | SCB_DFSR_HALTED_Msk (1UL /*<< SCB_DFSR_HALTED_Pos*/)

## 详细描述

Type definitions for the System Control Block Registers

## 宏定义说明

## ◆ SCB_AIRCR_ENDIANESS_Msk

#define SCB_AIRCR_ENDIANESS_Msk (1UL << SCB_AIRCR_ENDIANESS_Pos)

SCB AIRCR: ENDIANESS Mask

## ◆ SCB_AIRCR_ENDIANESS_Pos

#define SCB_AIRCR_ENDIANESS_Pos 15U

SCB AIRCR: ENDIANESS Position

## ◆ SCB_AIRCR_PRIGROUP_Msk

#define SCB_AIRCR_PRIGROUP_Msk (7UL << SCB_AIRCR_PRIGROUP_Pos)

SCB AIRCR: PRIGROUP Mask

## ◆ SCB_AIRCR_PRIGROUP_Pos

#define SCB_AIRCR_PRIGROUP_Pos 8U

SCB AIRCR: PRIGROUP Position

## ◆ SCB_AIRCR_SYSRESETREQ_Msk

#define SCB_AIRCR_SYSRESETREQ_Msk (1UL << SCB_AIRCR_SYSRESETREQ_Pos)

SCB AIRCR: SYSRESETREQ Mask

## ◆ SCB_AIRCR_SYSRESETREQ_Pos

#define SCB_AIRCR_SYSRESETREQ_Pos 2U

SCB AIRCR: SYSRESETREQ Position

## ◆ SCB_AIRCR_VECTCLRACTIVE_Msk

#define SCB_AIRCR_VECTCLRACTIVE_Msk (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)

SCB AIRCR: VECTCLRACTIVE Mask

## ◆ SCB_AIRCR_VECTCLRACTIVE_Pos

#define SCB_AIRCR_VECTCLRACTIVE_Pos 1U

SCB AIRCR: VECTCLRACTIVE Position

## ◆ SCB_AIRCR_VECTKEY_Msk

#define SCB_AIRCR_VECTKEY_Msk (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)

SCB AIRCR: VECTKEY Mask

## ◆ SCB_AIRCR_VECTKEY_Pos

#define SCB_AIRCR_VECTKEY_Pos 16U

SCB AIRCR: VECTKEY Position

## ◆ SCB_AIRCR_VECTKEYSTAT_Msk

#define SCB_AIRCR_VECTKEYSTAT_Msk (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)

SCB AIRCR: VECTKEYSTAT Mask

## ◆ SCB_AIRCR_VECTKEYSTAT_Pos

#define SCB_AIRCR_VECTKEYSTAT_Pos 16U

SCB AIRCR: VECTKEYSTAT Position

## ◆ SCB_AIRCR_VECTRESET_Msk

#define SCB_AIRCR_VECTRESET_Msk (1UL /*<< SCB_AIRCR_VECTRESET_Pos*/)

SCB AIRCR: VECTRESET Mask

## ◆ SCB_AIRCR_VECTRESET_Pos

#define SCB_AIRCR_VECTRESET_Pos 0U

SCB AIRCR: VECTRESET Position

## ◆ SCB_CCR_BFHFNMIGN_Msk

#define SCB_CCR_BFHFNMIGN_Msk (1UL << SCB_CCR_BFHFNMIGN_Pos)

SCB CCR: BFHFNMIGN Mask

## ◆ SCB_CCR_BFHFNMIGN_Pos

#define SCB_CCR_BFHFNMIGN_Pos 8U

SCB CCR: BFHFNMIGN Position

## ◆ SCB_CCR_DIV_0_TRP_Msk

#define SCB_CCR_DIV_0_TRP_Msk (1UL << SCB_CCR_DIV_0_TRP_Pos)

SCB CCR: DIV_0_TRP Mask

## ◆ SCB_CCR_DIV_0_TRP_Pos

#define SCB_CCR_DIV_0_TRP_Pos 4U

SCB CCR: DIV_0_TRP Position

## ◆ SCB_CCR_NONBASETHRDENA_Msk

#define SCB_CCR_NONBASETHRDENA_Msk (1UL /*<< SCB_CCR_NONBASETHRDENA_Pos*/)

SCB CCR: NONBASETHRDENA Mask

## ◆ SCB_CCR_NONBASETHRDENA_Pos

#define SCB_CCR_NONBASETHRDENA_Pos 0U

SCB CCR: NONBASETHRDENA Position

## ◆ SCB_CCR_STKALIGN_Msk

#define SCB_CCR_STKALIGN_Msk (1UL << SCB_CCR_STKALIGN_Pos)

SCB CCR: STKALIGN Mask

## ◆ SCB_CCR_STKALIGN_Pos

#define SCB_CCR_STKALIGN_Pos 9U

SCB CCR: STKALIGN Position

## ◆ SCB_CCR_UNALIGN_TRP_Msk

#define SCB_CCR_UNALIGN_TRP_Msk (1UL << SCB_CCR_UNALIGN_TRP_Pos)

SCB CCR: UNALIGN_TRP Mask

## ◆ SCB_CCR_UNALIGN_TRP_Pos

#define SCB_CCR_UNALIGN_TRP_Pos 3U

SCB CCR: UNALIGN_TRP Position

## ◆ SCB_CCR_USERSETMPEND_Msk

#define SCB_CCR_USERSETMPEND_Msk (1UL << SCB_CCR_USERSETMPEND_Pos)

SCB CCR: USERSETMPEND Mask

## ◆ SCB_CCR_USERSETMPEND_Pos

#define SCB_CCR_USERSETMPEND_Pos 1U

SCB CCR: USERSETMPEND Position

## ◆ SCB_CFSR_BFARVALID_Msk

#define SCB_CFSR_BFARVALID_Msk (1UL << SCB_CFSR_BFARVALID_Pos)

SCB CFSR (BFSR): BFARVALID Mask

## ◆ SCB_CFSR_BFARVALID_Pos

#define SCB_CFSR_BFARVALID_Pos (SCB_CFSR_BUSFAULTSR_Pos + 7U)

SCB CFSR (BFSR): BFARVALID Position

## ◆ SCB_CFSR_BUSFAULTSR_Msk

#define SCB_CFSR_BUSFAULTSR_Msk (0xFFUL << SCB_CFSR_BUSFAULTSR_Pos)

SCB CFSR: Bus Fault Status Register Mask

## ◆ SCB_CFSR_BUSFAULTSR_Pos

#define SCB_CFSR_BUSFAULTSR_Pos 8U

SCB CFSR: Bus Fault Status Register Position

## ◆ SCB_CFSR_DACCVIOL_Msk

#define SCB_CFSR_DACCVIOL_Msk (1UL << SCB_CFSR_DACCVIOL_Pos)

SCB CFSR (MMFSR): DACCVIOL Mask

## ◆ SCB_CFSR_DACCVIOL_Pos

#define SCB_CFSR_DACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 1U)

SCB CFSR (MMFSR): DACCVIOL Position

## ◆ SCB_CFSR_DIVBYZERO_Msk

#define SCB_CFSR_DIVBYZERO_Msk (1UL << SCB_CFSR_DIVBYZERO_Pos)

SCB CFSR (UFSR): DIVBYZERO Mask

## ◆ SCB_CFSR_DIVBYZERO_Pos

#define SCB_CFSR_DIVBYZERO_Pos (SCB_CFSR_USGFAULTSR_Pos + 9U)

SCB CFSR (UFSR): DIVBYZERO Position

## ◆ SCB_CFSR_IACCVIOL_Msk

#define SCB_CFSR_IACCVIOL_Msk (1UL /*<< SCB_CFSR_IACCVIOL_Pos*/)

SCB CFSR (MMFSR): IACCVIOL Mask

## ◆ SCB_CFSR_IACCVIOL_Pos

#define SCB_CFSR_IACCVIOL_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 0U)

SCB CFSR (MMFSR): IACCVIOL Position

## ◆ SCB_CFSR_IBUSERR_Msk

#define SCB_CFSR_IBUSERR_Msk (1UL << SCB_CFSR_IBUSERR_Pos)

SCB CFSR (BFSR): IBUSERR Mask

## ◆ SCB_CFSR_IBUSERR_Pos

#define SCB_CFSR_IBUSERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 0U)

SCB CFSR (BFSR): IBUSERR Position

## ◆ SCB_CFSR_IMPRECISERR_Msk

#define SCB_CFSR_IMPRECISERR_Msk (1UL << SCB_CFSR_IMPRECISERR_Pos)

SCB CFSR (BFSR): IMPRECISERR Mask

## ◆ SCB_CFSR_IMPRECISERR_Pos

#define SCB_CFSR_IMPRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 2U)

SCB CFSR (BFSR): IMPRECISERR Position

## ◆ SCB_CFSR_INVPC_Msk

#define SCB_CFSR_INVPC_Msk (1UL << SCB_CFSR_INVPC_Pos)

SCB CFSR (UFSR): INVPC Mask

## ◆ SCB_CFSR_INVPC_Pos

#define SCB_CFSR_INVPC_Pos (SCB_CFSR_USGFAULTSR_Pos + 2U)

SCB CFSR (UFSR): INVPC Position

## ◆ SCB_CFSR_INVSTATE_Msk

#define SCB_CFSR_INVSTATE_Msk (1UL << SCB_CFSR_INVSTATE_Pos)

SCB CFSR (UFSR): INVSTATE Mask

## ◆ SCB_CFSR_INVSTATE_Pos

#define SCB_CFSR_INVSTATE_Pos (SCB_CFSR_USGFAULTSR_Pos + 1U)

SCB CFSR (UFSR): INVSTATE Position

## ◆ SCB_CFSR_MEMFAULTSR_Msk

#define SCB_CFSR_MEMFAULTSR_Msk (0xFFUL /*<< SCB_CFSR_MEMFAULTSR_Pos*/)

SCB CFSR: Memory Manage Fault Status Register Mask

## ◆ SCB_CFSR_MEMFAULTSR_Pos

#define SCB_CFSR_MEMFAULTSR_Pos 0U

SCB CFSR: Memory Manage Fault Status Register Position

## ◆ SCB_CFSR_MMARVALID_Msk

#define SCB_CFSR_MMARVALID_Msk (1UL << SCB_CFSR_MMARVALID_Pos)

SCB CFSR (MMFSR): MMARVALID Mask

## ◆ SCB_CFSR_MMARVALID_Pos

#define SCB_CFSR_MMARVALID_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 7U)

SCB CFSR (MMFSR): MMARVALID Position

## ◆ SCB_CFSR_MSTKERR_Msk

#define SCB_CFSR_MSTKERR_Msk (1UL << SCB_CFSR_MSTKERR_Pos)

SCB CFSR (MMFSR): MSTKERR Mask

## ◆ SCB_CFSR_MSTKERR_Pos

#define SCB_CFSR_MSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 4U)

SCB CFSR (MMFSR): MSTKERR Position

## ◆ SCB_CFSR_MUNSTKERR_Msk

#define SCB_CFSR_MUNSTKERR_Msk (1UL << SCB_CFSR_MUNSTKERR_Pos)

SCB CFSR (MMFSR): MUNSTKERR Mask

## ◆ SCB_CFSR_MUNSTKERR_Pos

#define SCB_CFSR_MUNSTKERR_Pos (SCB_SHCSR_MEMFAULTACT_Pos + 3U)

SCB CFSR (MMFSR): MUNSTKERR Position

## ◆ SCB_CFSR_NOCP_Msk

#define SCB_CFSR_NOCP_Msk (1UL << SCB_CFSR_NOCP_Pos)

SCB CFSR (UFSR): NOCP Mask

## ◆ SCB_CFSR_NOCP_Pos

#define SCB_CFSR_NOCP_Pos (SCB_CFSR_USGFAULTSR_Pos + 3U)

SCB CFSR (UFSR): NOCP Position

## ◆ SCB_CFSR_PRECISERR_Msk

#define SCB_CFSR_PRECISERR_Msk (1UL << SCB_CFSR_PRECISERR_Pos)

SCB CFSR (BFSR): PRECISERR Mask

## ◆ SCB_CFSR_PRECISERR_Pos

#define SCB_CFSR_PRECISERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 1U)

SCB CFSR (BFSR): PRECISERR Position

## ◆ SCB_CFSR_STKERR_Msk

#define SCB_CFSR_STKERR_Msk (1UL << SCB_CFSR_STKERR_Pos)

SCB CFSR (BFSR): STKERR Mask

## ◆ SCB_CFSR_STKERR_Pos

#define SCB_CFSR_STKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 4U)

SCB CFSR (BFSR): STKERR Position

## ◆ SCB_CFSR_UNALIGNED_Msk

#define SCB_CFSR_UNALIGNED_Msk (1UL << SCB_CFSR_UNALIGNED_Pos)

SCB CFSR (UFSR): UNALIGNED Mask

## ◆ SCB_CFSR_UNALIGNED_Pos

#define SCB_CFSR_UNALIGNED_Pos (SCB_CFSR_USGFAULTSR_Pos + 8U)

SCB CFSR (UFSR): UNALIGNED Position

## ◆ SCB_CFSR_UNDEFINSTR_Msk

#define SCB_CFSR_UNDEFINSTR_Msk (1UL << SCB_CFSR_UNDEFINSTR_Pos)

SCB CFSR (UFSR): UNDEFINSTR Mask

## ◆ SCB_CFSR_UNDEFINSTR_Pos

#define SCB_CFSR_UNDEFINSTR_Pos (SCB_CFSR_USGFAULTSR_Pos + 0U)

SCB CFSR (UFSR): UNDEFINSTR Position

## ◆ SCB_CFSR_UNSTKERR_Msk

#define SCB_CFSR_UNSTKERR_Msk (1UL << SCB_CFSR_UNSTKERR_Pos)

SCB CFSR (BFSR): UNSTKERR Mask

## ◆ SCB_CFSR_UNSTKERR_Pos

#define SCB_CFSR_UNSTKERR_Pos (SCB_CFSR_BUSFAULTSR_Pos + 3U)

SCB CFSR (BFSR): UNSTKERR Position

## ◆ SCB_CFSR_USGFAULTSR_Msk

#define SCB_CFSR_USGFAULTSR_Msk (0xFFFFUL << SCB_CFSR_USGFAULTSR_Pos)

SCB CFSR: Usage Fault Status Register Mask

## ◆ SCB_CFSR_USGFAULTSR_Pos

#define SCB_CFSR_USGFAULTSR_Pos 16U

SCB CFSR: Usage Fault Status Register Position

## ◆ SCB_CPUID_ARCHITECTURE_Msk

#define SCB_CPUID_ARCHITECTURE_Msk (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)

SCB CPUID: ARCHITECTURE Mask

## ◆ SCB_CPUID_ARCHITECTURE_Pos

#define SCB_CPUID_ARCHITECTURE_Pos 16U

SCB CPUID: ARCHITECTURE Position

## ◆ SCB_CPUID_IMPLEMENTER_Msk

#define SCB_CPUID_IMPLEMENTER_Msk (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)

SCB CPUID: IMPLEMENTER Mask

## ◆ SCB_CPUID_IMPLEMENTER_Pos

#define SCB_CPUID_IMPLEMENTER_Pos 24U

SCB CPUID: IMPLEMENTER Position

## ◆ SCB_CPUID_PARTNO_Msk

#define SCB_CPUID_PARTNO_Msk (0xFFFUL << SCB_CPUID_PARTNO_Pos)

SCB CPUID: PARTNO Mask

## ◆ SCB_CPUID_PARTNO_Pos

#define SCB_CPUID_PARTNO_Pos 4U

SCB CPUID: PARTNO Position

## ◆ SCB_CPUID_REVISION_Msk

#define SCB_CPUID_REVISION_Msk (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)

SCB CPUID: REVISION Mask

## ◆ SCB_CPUID_REVISION_Pos

#define SCB_CPUID_REVISION_Pos 0U

SCB CPUID: REVISION Position

## ◆ SCB_CPUID_VARIANT_Msk

#define SCB_CPUID_VARIANT_Msk (0xFUL << SCB_CPUID_VARIANT_Pos)

SCB CPUID: VARIANT Mask

## ◆ SCB_CPUID_VARIANT_Pos

#define SCB_CPUID_VARIANT_Pos 20U

SCB CPUID: VARIANT Position

## ◆ SCB_DFSR_BKPT_Msk

#define SCB_DFSR_BKPT_Msk (1UL << SCB_DFSR_BKPT_Pos)

SCB DFSR: BKPT Mask

## ◆ SCB_DFSR_BKPT_Pos

#define SCB_DFSR_BKPT_Pos 1U

SCB DFSR: BKPT Position

## ◆ SCB_DFSR_DWTTRAP_Msk

#define SCB_DFSR_DWTTRAP_Msk (1UL << SCB_DFSR_DWTTRAP_Pos)

SCB DFSR: DWTTRAP Mask

## ◆ SCB_DFSR_DWTTRAP_Pos

#define SCB_DFSR_DWTTRAP_Pos 2U

SCB DFSR: DWTTRAP Position

## ◆ SCB_DFSR_EXTERNAL_Msk

#define SCB_DFSR_EXTERNAL_Msk (1UL << SCB_DFSR_EXTERNAL_Pos)

SCB DFSR: EXTERNAL Mask

## ◆ SCB_DFSR_EXTERNAL_Pos

#define SCB_DFSR_EXTERNAL_Pos 4U

SCB DFSR: EXTERNAL Position

## ◆ SCB_DFSR_HALTED_Msk

#define SCB_DFSR_HALTED_Msk (1UL /*<< SCB_DFSR_HALTED_Pos*/)

SCB DFSR: HALTED Mask

## ◆ SCB_DFSR_HALTED_Pos

#define SCB_DFSR_HALTED_Pos 0U

SCB DFSR: HALTED Position

## ◆ SCB_DFSR_VCATCH_Msk

#define SCB_DFSR_VCATCH_Msk (1UL << SCB_DFSR_VCATCH_Pos)

SCB DFSR: VCATCH Mask

## ◆ SCB_DFSR_VCATCH_Pos

#define SCB_DFSR_VCATCH_Pos 3U

SCB DFSR: VCATCH Position

## ◆ SCB_HFSR_DEBUGEVT_Msk

#define SCB_HFSR_DEBUGEVT_Msk (1UL << SCB_HFSR_DEBUGEVT_Pos)

SCB HFSR: DEBUGEVT Mask

## ◆ SCB_HFSR_DEBUGEVT_Pos

#define SCB_HFSR_DEBUGEVT_Pos 31U

SCB HFSR: DEBUGEVT Position

## ◆ SCB_HFSR_FORCED_Msk

#define SCB_HFSR_FORCED_Msk (1UL << SCB_HFSR_FORCED_Pos)

SCB HFSR: FORCED Mask

## ◆ SCB_HFSR_FORCED_Pos

#define SCB_HFSR_FORCED_Pos 30U

SCB HFSR: FORCED Position

## ◆ SCB_HFSR_VECTTBL_Msk

#define SCB_HFSR_VECTTBL_Msk (1UL << SCB_HFSR_VECTTBL_Pos)

SCB HFSR: VECTTBL Mask

## ◆ SCB_HFSR_VECTTBL_Pos

#define SCB_HFSR_VECTTBL_Pos 1U

SCB HFSR: VECTTBL Position

## ◆ SCB_ICSR_ISRPENDING_Msk

#define SCB_ICSR_ISRPENDING_Msk (1UL << SCB_ICSR_ISRPENDING_Pos)

SCB ICSR: ISRPENDING Mask

## ◆ SCB_ICSR_ISRPENDING_Pos

#define SCB_ICSR_ISRPENDING_Pos 22U

SCB ICSR: ISRPENDING Position

## ◆ SCB_ICSR_ISRPREEMPT_Msk

#define SCB_ICSR_ISRPREEMPT_Msk (1UL << SCB_ICSR_ISRPREEMPT_Pos)

SCB ICSR: ISRPREEMPT Mask

## ◆ SCB_ICSR_ISRPREEMPT_Pos

#define SCB_ICSR_ISRPREEMPT_Pos 23U

SCB ICSR: ISRPREEMPT Position

## ◆ SCB_ICSR_NMIPENDSET_Msk

#define SCB_ICSR_NMIPENDSET_Msk (1UL << SCB_ICSR_NMIPENDSET_Pos)

SCB ICSR: NMIPENDSET Mask

## ◆ SCB_ICSR_NMIPENDSET_Pos

#define SCB_ICSR_NMIPENDSET_Pos 31U

SCB ICSR: NMIPENDSET Position

## ◆ SCB_ICSR_PENDSTCLR_Msk

#define SCB_ICSR_PENDSTCLR_Msk (1UL << SCB_ICSR_PENDSTCLR_Pos)

SCB ICSR: PENDSTCLR Mask

## ◆ SCB_ICSR_PENDSTCLR_Pos

#define SCB_ICSR_PENDSTCLR_Pos 25U

SCB ICSR: PENDSTCLR Position

## ◆ SCB_ICSR_PENDSTSET_Msk

#define SCB_ICSR_PENDSTSET_Msk (1UL << SCB_ICSR_PENDSTSET_Pos)

SCB ICSR: PENDSTSET Mask

## ◆ SCB_ICSR_PENDSTSET_Pos

#define SCB_ICSR_PENDSTSET_Pos 26U

SCB ICSR: PENDSTSET Position

## ◆ SCB_ICSR_PENDSVCLR_Msk

#define SCB_ICSR_PENDSVCLR_Msk (1UL << SCB_ICSR_PENDSVCLR_Pos)

SCB ICSR: PENDSVCLR Mask

## ◆ SCB_ICSR_PENDSVCLR_Pos

#define SCB_ICSR_PENDSVCLR_Pos 27U

SCB ICSR: PENDSVCLR Position

## ◆ SCB_ICSR_PENDSVSET_Msk

#define SCB_ICSR_PENDSVSET_Msk (1UL << SCB_ICSR_PENDSVSET_Pos)

SCB ICSR: PENDSVSET Mask

## ◆ SCB_ICSR_PENDSVSET_Pos

#define SCB_ICSR_PENDSVSET_Pos 28U

SCB ICSR: PENDSVSET Position

## ◆ SCB_ICSR_RETTOBASE_Msk

#define SCB_ICSR_RETTOBASE_Msk (1UL << SCB_ICSR_RETTOBASE_Pos)

SCB ICSR: RETTOBASE Mask

## ◆ SCB_ICSR_RETTOBASE_Pos

#define SCB_ICSR_RETTOBASE_Pos 11U

SCB ICSR: RETTOBASE Position

## ◆ SCB_ICSR_VECTACTIVE_Msk

#define SCB_ICSR_VECTACTIVE_Msk (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)

SCB ICSR: VECTACTIVE Mask

## ◆ SCB_ICSR_VECTACTIVE_Pos

#define SCB_ICSR_VECTACTIVE_Pos 0U

SCB ICSR: VECTACTIVE Position

## ◆ SCB_ICSR_VECTPENDING_Msk

#define SCB_ICSR_VECTPENDING_Msk (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)

SCB ICSR: VECTPENDING Mask

## ◆ SCB_ICSR_VECTPENDING_Pos

#define SCB_ICSR_VECTPENDING_Pos 12U

SCB ICSR: VECTPENDING Position

## ◆ SCB_SCR_SEVONPEND_Msk

#define SCB_SCR_SEVONPEND_Msk (1UL << SCB_SCR_SEVONPEND_Pos)

SCB SCR: SEVONPEND Mask

## ◆ SCB_SCR_SEVONPEND_Pos

#define SCB_SCR_SEVONPEND_Pos 4U

SCB SCR: SEVONPEND Position

## ◆ SCB_SCR_SLEEPDEEP_Msk

#define SCB_SCR_SLEEPDEEP_Msk (1UL << SCB_SCR_SLEEPDEEP_Pos)

SCB SCR: SLEEPDEEP Mask

## ◆ SCB_SCR_SLEEPDEEP_Pos

#define SCB_SCR_SLEEPDEEP_Pos 2U

SCB SCR: SLEEPDEEP Position

## ◆ SCB_SCR_SLEEPONEXIT_Msk

#define SCB_SCR_SLEEPONEXIT_Msk (1UL << SCB_SCR_SLEEPONEXIT_Pos)

SCB SCR: SLEEPONEXIT Mask

## ◆ SCB_SCR_SLEEPONEXIT_Pos

#define SCB_SCR_SLEEPONEXIT_Pos 1U

SCB SCR: SLEEPONEXIT Position

## ◆ SCB_SHCSR_BUSFAULTACT_Msk

#define SCB_SHCSR_BUSFAULTACT_Msk (1UL << SCB_SHCSR_BUSFAULTACT_Pos)

SCB SHCSR: BUSFAULTACT Mask

## ◆ SCB_SHCSR_BUSFAULTACT_Pos

#define SCB_SHCSR_BUSFAULTACT_Pos 1U

SCB SHCSR: BUSFAULTACT Position

## ◆ SCB_SHCSR_BUSFAULTENA_Msk

#define SCB_SHCSR_BUSFAULTENA_Msk (1UL << SCB_SHCSR_BUSFAULTENA_Pos)

SCB SHCSR: BUSFAULTENA Mask

## ◆ SCB_SHCSR_BUSFAULTENA_Pos

#define SCB_SHCSR_BUSFAULTENA_Pos 17U

SCB SHCSR: BUSFAULTENA Position

## ◆ SCB_SHCSR_BUSFAULTPENDED_Msk

#define SCB_SHCSR_BUSFAULTPENDED_Msk (1UL << SCB_SHCSR_BUSFAULTPENDED_Pos)

SCB SHCSR: BUSFAULTPENDED Mask

## ◆ SCB_SHCSR_BUSFAULTPENDED_Pos

#define SCB_SHCSR_BUSFAULTPENDED_Pos 14U

SCB SHCSR: BUSFAULTPENDED Position

## ◆ SCB_SHCSR_MEMFAULTACT_Msk

#define SCB_SHCSR_MEMFAULTACT_Msk (1UL /*<< SCB_SHCSR_MEMFAULTACT_Pos*/)

SCB SHCSR: MEMFAULTACT Mask

## ◆ SCB_SHCSR_MEMFAULTACT_Pos

#define SCB_SHCSR_MEMFAULTACT_Pos 0U

SCB SHCSR: MEMFAULTACT Position

## ◆ SCB_SHCSR_MEMFAULTENA_Msk

#define SCB_SHCSR_MEMFAULTENA_Msk (1UL << SCB_SHCSR_MEMFAULTENA_Pos)

SCB SHCSR: MEMFAULTENA Mask

## ◆ SCB_SHCSR_MEMFAULTENA_Pos

#define SCB_SHCSR_MEMFAULTENA_Pos 16U

SCB SHCSR: MEMFAULTENA Position

## ◆ SCB_SHCSR_MEMFAULTPENDED_Msk

#define SCB_SHCSR_MEMFAULTPENDED_Msk (1UL << SCB_SHCSR_MEMFAULTPENDED_Pos)

SCB SHCSR: MEMFAULTPENDED Mask

## ◆ SCB_SHCSR_MEMFAULTPENDED_Pos

#define SCB_SHCSR_MEMFAULTPENDED_Pos 13U

SCB SHCSR: MEMFAULTPENDED Position

## ◆ SCB_SHCSR_MONITORACT_Msk

#define SCB_SHCSR_MONITORACT_Msk (1UL << SCB_SHCSR_MONITORACT_Pos)

SCB SHCSR: MONITORACT Mask

## ◆ SCB_SHCSR_MONITORACT_Pos

#define SCB_SHCSR_MONITORACT_Pos 8U

SCB SHCSR: MONITORACT Position

## ◆ SCB_SHCSR_PENDSVACT_Msk

#define SCB_SHCSR_PENDSVACT_Msk (1UL << SCB_SHCSR_PENDSVACT_Pos)

SCB SHCSR: PENDSVACT Mask

## ◆ SCB_SHCSR_PENDSVACT_Pos

#define SCB_SHCSR_PENDSVACT_Pos 10U

SCB SHCSR: PENDSVACT Position

## ◆ SCB_SHCSR_SVCALLACT_Msk

#define SCB_SHCSR_SVCALLACT_Msk (1UL << SCB_SHCSR_SVCALLACT_Pos)

SCB SHCSR: SVCALLACT Mask

## ◆ SCB_SHCSR_SVCALLACT_Pos

#define SCB_SHCSR_SVCALLACT_Pos 7U

SCB SHCSR: SVCALLACT Position

## ◆ SCB_SHCSR_SVCALLPENDED_Msk

#define SCB_SHCSR_SVCALLPENDED_Msk (1UL << SCB_SHCSR_SVCALLPENDED_Pos)

SCB SHCSR: SVCALLPENDED Mask

## ◆ SCB_SHCSR_SVCALLPENDED_Pos

#define SCB_SHCSR_SVCALLPENDED_Pos 15U

SCB SHCSR: SVCALLPENDED Position

## ◆ SCB_SHCSR_SYSTICKACT_Msk

#define SCB_SHCSR_SYSTICKACT_Msk (1UL << SCB_SHCSR_SYSTICKACT_Pos)

SCB SHCSR: SYSTICKACT Mask

## ◆ SCB_SHCSR_SYSTICKACT_Pos

#define SCB_SHCSR_SYSTICKACT_Pos 11U

SCB SHCSR: SYSTICKACT Position

## ◆ SCB_SHCSR_USGFAULTACT_Msk

#define SCB_SHCSR_USGFAULTACT_Msk (1UL << SCB_SHCSR_USGFAULTACT_Pos)

SCB SHCSR: USGFAULTACT Mask

## ◆ SCB_SHCSR_USGFAULTACT_Pos

#define SCB_SHCSR_USGFAULTACT_Pos 3U

SCB SHCSR: USGFAULTACT Position

## ◆ SCB_SHCSR_USGFAULTENA_Msk

#define SCB_SHCSR_USGFAULTENA_Msk (1UL << SCB_SHCSR_USGFAULTENA_Pos)

SCB SHCSR: USGFAULTENA Mask

## ◆ SCB_SHCSR_USGFAULTENA_Pos

#define SCB_SHCSR_USGFAULTENA_Pos 18U

SCB SHCSR: USGFAULTENA Position

## ◆ SCB_SHCSR_USGFAULTPENDED_Msk

#define SCB_SHCSR_USGFAULTPENDED_Msk (1UL << SCB_SHCSR_USGFAULTPENDED_Pos)

SCB SHCSR: USGFAULTPENDED Mask

## ◆ SCB_SHCSR_USGFAULTPENDED_Pos

#define SCB_SHCSR_USGFAULTPENDED_Pos 12U

SCB SHCSR: USGFAULTPENDED Position

## ◆ SCB_VTOR_TBLOFF_Msk

#define SCB_VTOR_TBLOFF_Msk (0x1FFFFFFUL << SCB_VTOR_TBLOFF_Pos)

SCB VTOR: TBLOFF Mask

## ◆ SCB_VTOR_TBLOFF_Pos

#define SCB_VTOR_TBLOFF_Pos 7U

SCB VTOR: TBLOFF Position