MG32F10x Standard Peripherals Firmware Library

NVIC_DMA_WFIMode example

      *************** (C) COPYRIGHT 2020 - 2023 megawin Technology ***************
      * @file    NVIC/NVIC_DMA_WFIMode/readme.txt
      * @author  megawin Application Team
      * @version V0.1.10
      * @date    05-January-2023
      * @brief   Description of the NVIC NVIC_DMA_WFIMode example.
      ******************************************************************************
      * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
      * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
      * TIME. AS A RESULT, MEGAWIN SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
      * INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM
      * THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
      * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
      ******************************************************************************

例程描述

本例程演示在启用DMA传输的情况下系统进入WFI模式，如何通过DMA传输结束中断从该模式唤醒。

本例程系统时钟工作在96Mhz，通过PLL配置产生。PLL时钟源是外部8Mhz晶振。APB1的分频比是1，APB2的分频比是1。

按下按键（PB6）令内核进入WFI模式，LED1停止切换。要从WFI模式唤醒， 您必须将ASCII序列（0, 1, 2, 3, 4, 5, 6, 7, 8, 9）发送到UART1。 DMAC将这些字节从UART1接收数据寄存器传输到预定义的缓冲区，然后生成一个中断， 使系统退出WFI模式，LED1重新开始切换。如果收到正确的序列，则LED2点亮，否则LED2熄灭。

目录内容

- NVIC/NVIC_DMA_WFIMode/NVIC_DMA_WFIMode.uvprojx MDK5工程文件
- NVIC/NVIC_DMA_WFIMode/NVIC_DMA_WFIMode.uvoptx MDK5工程配置文件
- NVIC/NVIC_DMA_WFIMode/JLinkSettings.ini Jlink配置文件
- NVIC/NVIC_DMA_WFIMode/main.c 主程序

硬件和软件环境

- 硬件平台搭建
  - HSE 连接外部8MHz晶振
  - 芯片管脚连接如下：
    - PB14 管脚连接到 LED1
    - PB13 管脚连接到 LED2
    - PB6 管脚连接到 KEY

如何使用？

为了使程序工作，您必须执行以下操作 :

- 使用 MDK5 打开此例程文件夹中的 NVIC_DMA_WFIMode.uvprojx 工程
- 重新编译该工程并下载到目标存储器中

- 运行此例程

  ###
  © COPYRIGHT 2020 - 2023 megawin Technology