MG32F10x Standard Peripherals Firmware Library

模块 | 宏定义 | 枚举
GPIO_Exported_Constants
MG32F10x_StdPeriph_Driver » GPIO

## 模块
| GPIO_Pins_define
| GPIO_Port_Sources
| GPIO_Pin_sources
| GPIO_MODE_define
| GPIO_OTYPE_define
| GPIO_SPEED_define
| GPIO_PUPD_define
| GPIO_AF_define

## 宏定义
#define | IS_GPIO_ALL_PERIPH(PERIPH)
#define | IS_GPIO_BIT_ACTION(ACTION) (((ACTION) == Bit_RESET) || ((ACTION) == Bit_SET))

## 枚举
enum | BitAction { Bit_RESET = 0, Bit_SET }
| GPIO Bit SET and Bit RESET enumeration

## 详细描述

## 宏定义说明

## ◆ IS_GPIO_ALL_PERIPH

#define IS_GPIO_ALL_PERIPH | ( |  | PERIPH | ) |

值:
(((PERIPH) == GPIOA) || \
((PERIPH) == GPIOB) || \
((PERIPH) == GPIOC) || \
((PERIPH) == GPIOD))