MG32F10x Standard Peripherals Firmware Library

模块 | 函数
I2S
MG32F10x_StdPeriph_Driver

I2S driver modules 更多...

## 模块
| I2S_Exported_Constants
| I2S_Private_Functions

## 函数
void | I2S_DeInit (void)
| Deinitializes the I2S peripheral registers to their default reset values. 更多...
void | I2S_Cmd (FunctionalState NewState)
| Enables or disables the specified I2S peripheral. 更多...
void | I2S_ReceiverCmd (FunctionalState NewState)
| Enables or disables the I2S receiver block. 更多...
void | I2S_TransmitterCmd (FunctionalState NewState)
| Enables or disables the I2S transmitter block. 更多...
void | I2S_ClockConfig (uint32_t I2S_WordSelectSize, uint32_t I2S_SclkGate)
| Configures I2S Clock Generation block. 更多...
void | I2S_ClockCmd (FunctionalState NewState)
| Enables or disables the I2S clock generation block. 更多...
void | I2S_ReceiverFIFOFlush (void)
| Flushes all the RX FIFOs. 更多...
void | I2S_TransmitterFIFOFlush (void)
| Flushes all the TX FIFOs. 更多...
uint32_t | I2S_Channel_ReadLeftData (uint32_t I2S_Channel)
| Read the left stereo data from Rx FIFO. 更多...
uint32_t | I2S_Channel_ReadRightData (uint32_t I2S_Channel)
| Read the right stereo data from Rx FIFO. 更多...
void | I2S_Channel_WriteLeftData (uint32_t I2S_Channel, uint32_t LeftData)
| Write the left stereo data to Tx FIFO. 更多...
void | I2S_Channel_WriteRightData (uint32_t I2S_Channel, uint32_t RightData)
| Write the right stereo data to Tx FIFO. 更多...
void | I2S_Channel_ReceiveCmd (uint32_t I2S_Channel, FunctionalState NewState)
| Enables or disables the receive channel. 更多...
void | I2S_Channel_TransmitCmd (uint32_t I2S_Channel, FunctionalState NewState)
| Enables or disables the transmit channel. 更多...
void | I2S_Channel_ReceiveConfig (uint32_t I2S_Channel, uint32_t I2S_DataFormat)
| Configures the desired data resolution of the receiver. 更多...
void | I2S_Channel_TransmitConfig (uint32_t I2S_Channel, uint32_t I2S_DataFormat)
| Configures the data resolution of the transmitter. 更多...
void | I2S_Channel_ITConfig (uint32_t I2S_Channel, uint8_t I2S_IT, FunctionalState NewState)
| Enables or disables the specified I2S interrupts. 更多...
ITStatus | I2S_Channel_GetITStatus (uint32_t I2S_Channel, uint8_t I2S_IT)
| Checks whether the specified I2S interrupt has occurred or not. 更多...
void | I2S_Channel_ClearITPendingBit (uint32_t I2S_Channel, uint8_t I2S_IT)
| Clears the I2S interrupt pending bits. 更多...
void | I2S_Channel_ReceiveFIFOConfig (uint32_t I2S_Channel, uint8_t Threshold)
| Configures the Rx FIFO threshold. 更多...
void | I2S_Channel_TransmitFIFOConfig (uint32_t I2S_Channel, uint8_t Threshold)
| Configures the Tx FIFO threshold. 更多...
void | I2S_Channel_ReceiveFIFOFlush (uint32_t I2S_Channel)
| Flushes the corresponding RX FIFO. 更多...
void | I2S_Channel_TransmitFIFOFlush (uint32_t I2S_Channel)
| Flushes the corresponding TX FIFO. 更多...

## 详细描述

I2S driver modules

## 函数说明

## ◆ I2S_Channel_ClearITPendingBit()

void I2S_Channel_ClearITPendingBit | ( | uint32_t | I2S_Channel,
|  | uint8_t | I2S_IT
| ) |  |

Clears the I2S interrupt pending bits.

参数

  I2S_Channel | specifies the selected I2S channel.
  I2S_IT | specifies the interrupt pending bit to clear. This parameter can be a combination of the following values: I2S_IT_RXFO: RX FIFO Overrun interrupt. I2S_IT_TXFO: TX FIFO Overrun interrupt.

返回
  None.

## ◆ I2S_Channel_GetITStatus()

ITStatus I2S_Channel_GetITStatus | ( | uint32_t | I2S_Channel,
|  | uint8_t | I2S_IT
| ) |  |

Checks whether the specified I2S interrupt has occurred or not.

参数

  I2S_Channel | specifies the selected I2S channel.
  I2S_IT | specifies the I2S interrupt source to check. This parameter can be one of the following values: I2S_IT_RXDA: RX FIFO Data Available interrupt. I2S_IT_RXFO: RX FIFO Overrun interrupt. I2S_IT_TXFE: TX FIFO Empty interrupt. I2S_IT_TXFO: TX FIFO Overrun interrupt.

返回
  The new state of I2S_IT (SET or RESET).

## ◆ I2S_Channel_ITConfig()

void I2S_Channel_ITConfig | ( | uint32_t | I2S_Channel,
|  | uint8_t | I2S_IT,
|  | FunctionalState | NewState
| ) |  |

Enables or disables the specified I2S interrupts.

参数

  I2S_Channel | specifies the selected I2S channel.
  I2S_IT | specifies the I2S interrupt source to be enabled or disabled. This parameter can be a combination of the following values: I2S_IT_RXDA: RX FIFO Data Available interrupt. I2S_IT_RXFO: RX FIFO Overrun interrupt. I2S_IT_TXFE: TX FIFO Empty interrupt. I2S_IT_TXFO: TX FIFO Overrun interrupt.
  NewState | new state of the specified I2S interrupt. This parameter can be: ENABLE or DISABLE.

返回
  None.

## ◆ I2S_Channel_ReadLeftData()

uint32_t I2S_Channel_ReadLeftData | ( | uint32_t | I2S_Channel | ) |

Read the left stereo data from Rx FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.

返回
  The left stereo data.

## ◆ I2S_Channel_ReadRightData()

uint32_t I2S_Channel_ReadRightData | ( | uint32_t | I2S_Channel | ) |

Read the right stereo data from Rx FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.

返回
  The right stereo data.

## ◆ I2S_Channel_ReceiveCmd()

void I2S_Channel_ReceiveCmd | ( | uint32_t | I2S_Channel,
|  | FunctionalState | NewState
| ) |  |

Enables or disables the receive channel.

参数

  I2S_Channel | specifies the selected I2S channel.
  NewState | new state of the receive channel. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_Channel_ReceiveConfig()

void I2S_Channel_ReceiveConfig | ( | uint32_t | I2S_Channel,
|  | uint32_t | I2S_DataFormat
| ) |  |

Configures the desired data resolution of the receiver.

参数

  I2S_Channel | specifies the selected I2S channel.
  I2S_DataFormat | specifies the desired data resolution. This parameter can be one of the following values: I2S_DataFormat_Ignore I2S_DataFormat_12b I2S_DataFormat_16b I2S_DataFormat_20b I2S_DataFormat_24b I2S_DataFormat_32b

返回
  None

## ◆ I2S_Channel_ReceiveFIFOConfig()

void I2S_Channel_ReceiveFIFOConfig | ( | uint32_t | I2S_Channel,
|  | uint8_t | Threshold
| ) |  |

Configures the Rx FIFO threshold.

参数

  I2S_Channel | specifies the selected I2S channel.
  Threshold | The Rx FIFO threshold to set.

注解
  The RX FIFO Data Available interrupt will trigger when the level > Threshold.

返回
  None.

## ◆ I2S_Channel_ReceiveFIFOFlush()

void I2S_Channel_ReceiveFIFOFlush | ( | uint32_t | I2S_Channel | ) |

Flushes the corresponding RX FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.

返回
  None

## ◆ I2S_Channel_TransmitCmd()

void I2S_Channel_TransmitCmd | ( | uint32_t | I2S_Channel,
|  | FunctionalState | NewState
| ) |  |

Enables or disables the transmit channel.

参数

  I2S_Channel | specifies the selected I2S channel.
  NewState | new state of the transmit channel. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_Channel_TransmitConfig()

void I2S_Channel_TransmitConfig | ( | uint32_t | I2S_Channel,
|  | uint32_t | I2S_DataFormat
| ) |  |

Configures the data resolution of the transmitter.

参数

  I2S_Channel | specifies the selected I2S channel.
  I2S_DataFormat | specifies the data resolution. This parameter can be one of the following values: I2S_DataFormat_Ignore I2S_DataFormat_12b I2S_DataFormat_16b I2S_DataFormat_20b I2S_DataFormat_24b I2S_DataFormat_32b

返回
  None

## ◆ I2S_Channel_TransmitFIFOConfig()

void I2S_Channel_TransmitFIFOConfig | ( | uint32_t | I2S_Channel,
|  | uint8_t | Threshold
| ) |  |

Configures the Tx FIFO threshold.

参数

  I2S_Channel | specifies the selected I2S channel.
  Threshold | The Tx FIFO threshold to set.

注解
  The TX FIFO Empty interrupt will trigger when the level <= Threshold.

返回
  None.

## ◆ I2S_Channel_TransmitFIFOFlush()

void I2S_Channel_TransmitFIFOFlush | ( | uint32_t | I2S_Channel | ) |

Flushes the corresponding TX FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.

返回
  None

## ◆ I2S_Channel_WriteLeftData()

void I2S_Channel_WriteLeftData | ( | uint32_t | I2S_Channel,
|  | uint32_t | LeftData
| ) |  |

Write the left stereo data to Tx FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.
  LeftData | The left stereo data to write.

返回
  None

## ◆ I2S_Channel_WriteRightData()

void I2S_Channel_WriteRightData | ( | uint32_t | I2S_Channel,
|  | uint32_t | RightData
| ) |  |

Write the right stereo data to Tx FIFO.

参数

  I2S_Channel | specifies the selected I2S channel.
  RightData | The right stereo data to write.

返回
  None

## ◆ I2S_ClockCmd()

void I2S_ClockCmd | ( | FunctionalState | NewState | ) |

Enables or disables the I2S clock generation block.

参数

  NewState | new state of the clock generation block. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_ClockConfig()

void I2S_ClockConfig | ( | uint32_t | I2S_WordSelectSize,
|  | uint32_t | I2S_SclkGate
| ) |  |

Configures I2S Clock Generation block.

参数

  I2S_WordSelectSize | specifies the number of sclk cycles for which the word select line stays in the left or right sample mode. This parameter can be one of the following values: I2S_WordSelectSize_16 I2S_WordSelectSize_24 I2S_WordSelectSize_32
  I2S_SclkGate | specifies the gating of sclk. This parameter can be one of the following values: I2S_SclkGate_None I2S_SclkGate_12 I2S_SclkGate_16 I2S_SclkGate_20 I2S_SclkGate_24

返回
  None

## ◆ I2S_Cmd()

void I2S_Cmd | ( | FunctionalState | NewState | ) |

Enables or disables the specified I2S peripheral.

参数

  NewState | new state of the I2S peripheral. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_DeInit()

void I2S_DeInit | ( | void |  | ) |

Deinitializes the I2S peripheral registers to their default reset values.

返回
  None

## ◆ I2S_ReceiverCmd()

void I2S_ReceiverCmd | ( | FunctionalState | NewState | ) |

Enables or disables the I2S receiver block.

参数

  NewState | new state of the receiver block. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_ReceiverFIFOFlush()

void I2S_ReceiverFIFOFlush | ( | void |  | ) |

Flushes all the RX FIFOs.

返回
  None

## ◆ I2S_TransmitterCmd()

void I2S_TransmitterCmd | ( | FunctionalState | NewState | ) |

Enables or disables the I2S transmitter block.

参数

  NewState | new state of the transmitter block. This parameter can be: ENABLE or DISABLE.

返回
  None

## ◆ I2S_TransmitterFIFOFlush()

void I2S_TransmitterFIFOFlush | ( | void |  | ) |

Flushes all the TX FIFOs.

返回
  None