MG32F10x Standard Peripherals Firmware Library

宏定义
ADC_injected_channel_selection
MG32F10x_StdPeriph_Driver » ADC » ADC_Exported_Constants

## 宏定义
#define | ADC_InjectedChannel_1 ((uint8_t)0x14)
#define | ADC_InjectedChannel_2 ((uint8_t)0x18)
#define | ADC_InjectedChannel_3 ((uint8_t)0x1C)
#define | ADC_InjectedChannel_4 ((uint8_t)0x20)
#define | IS_ADC_INJECTED_CHANNEL(CHANNEL)

## 详细描述

## 宏定义说明

## ◆ IS_ADC_INJECTED_CHANNEL

#define IS_ADC_INJECTED_CHANNEL | ( |  | CHANNEL | ) |

值:
(((CHANNEL) == ADC_InjectedChannel_1) || \
((CHANNEL) == ADC_InjectedChannel_2) || \
((CHANNEL) == ADC_InjectedChannel_3) || \
((CHANNEL) == ADC_InjectedChannel_4))