MG32F10x Standard Peripherals Firmware Library

结构体 | 宏定义
System Controls not in SCB (SCnSCB)
Defines and Type Definitions

Type definitions for the System Control and ID Register not in the SCB 更多...

## 结构体
struct | SCnSCB_Type
| Structure type to access the System Control and ID Register not in the SCB. 更多...

## 宏定义
#define | SCnSCB_ICTR_INTLINESNUM_Pos 0U
#define | SCnSCB_ICTR_INTLINESNUM_Msk (0xFUL /*<< SCnSCB_ICTR_INTLINESNUM_Pos*/)
#define | SCnSCB_ACTLR_DISFOLD_Pos 2U
#define | SCnSCB_ACTLR_DISFOLD_Msk (1UL << SCnSCB_ACTLR_DISFOLD_Pos)
#define | SCnSCB_ACTLR_DISDEFWBUF_Pos 1U
#define | SCnSCB_ACTLR_DISDEFWBUF_Msk (1UL << SCnSCB_ACTLR_DISDEFWBUF_Pos)
#define | SCnSCB_ACTLR_DISMCYCINT_Pos 0U
#define | SCnSCB_ACTLR_DISMCYCINT_Msk (1UL /*<< SCnSCB_ACTLR_DISMCYCINT_Pos*/)

## 详细描述

Type definitions for the System Control and ID Register not in the SCB

## 宏定义说明

## ◆ SCnSCB_ACTLR_DISDEFWBUF_Msk

#define SCnSCB_ACTLR_DISDEFWBUF_Msk (1UL << SCnSCB_ACTLR_DISDEFWBUF_Pos)

ACTLR: DISDEFWBUF Mask

## ◆ SCnSCB_ACTLR_DISDEFWBUF_Pos

#define SCnSCB_ACTLR_DISDEFWBUF_Pos 1U

ACTLR: DISDEFWBUF Position

## ◆ SCnSCB_ACTLR_DISFOLD_Msk

#define SCnSCB_ACTLR_DISFOLD_Msk (1UL << SCnSCB_ACTLR_DISFOLD_Pos)

ACTLR: DISFOLD Mask

## ◆ SCnSCB_ACTLR_DISFOLD_Pos

#define SCnSCB_ACTLR_DISFOLD_Pos 2U

ACTLR: DISFOLD Position

## ◆ SCnSCB_ACTLR_DISMCYCINT_Msk

#define SCnSCB_ACTLR_DISMCYCINT_Msk (1UL /*<< SCnSCB_ACTLR_DISMCYCINT_Pos*/)

ACTLR: DISMCYCINT Mask

## ◆ SCnSCB_ACTLR_DISMCYCINT_Pos

#define SCnSCB_ACTLR_DISMCYCINT_Pos 0U

ACTLR: DISMCYCINT Position

## ◆ SCnSCB_ICTR_INTLINESNUM_Msk

#define SCnSCB_ICTR_INTLINESNUM_Msk (0xFUL /*<< SCnSCB_ICTR_INTLINESNUM_Pos*/)

ICTR: INTLINESNUM Mask

## ◆ SCnSCB_ICTR_INTLINESNUM_Pos

#define SCnSCB_ICTR_INTLINESNUM_Pos 0U

ICTR: INTLINESNUM Position