MG32F10x Standard Peripherals Firmware Library

结构体 | 宏定义 | 枚举 | 函数
mg32f10x_exti.h 文件参考

This file contains all the functions prototypes for the EXTI firmware library. 更多...

`#include "mg32f10x.h"`

浏览源代码.

## 结构体
struct | EXTI_InitTypeDef
| EXTI Init Structure definition 更多...

## 宏定义
#define | IS_EXTI_MODE(MODE) (((MODE) == EXTI_Mode_Interrupt) || ((MODE) == EXTI_Mode_Event))
#define | IS_EXTI_TRIGGER(TRIGGER)
#define | EXTI_Line0 ((uint32_t)0x00001)
#define | EXTI_Line1 ((uint32_t)0x00002)
#define | EXTI_Line2 ((uint32_t)0x00004)
#define | EXTI_Line3 ((uint32_t)0x00008)
#define | EXTI_Line4 ((uint32_t)0x00010)
#define | EXTI_Line5 ((uint32_t)0x00020)
#define | EXTI_Line6 ((uint32_t)0x00040)
#define | EXTI_Line7 ((uint32_t)0x00080)
#define | EXTI_Line8 ((uint32_t)0x00100)
#define | EXTI_Line9 ((uint32_t)0x00200)
#define | EXTI_Line10 ((uint32_t)0x00400)
#define | EXTI_Line11 ((uint32_t)0x00800)
#define | EXTI_Line12 ((uint32_t)0x01000)
#define | EXTI_Line13 ((uint32_t)0x02000)
#define | EXTI_Line14 ((uint32_t)0x04000)
#define | EXTI_Line15 ((uint32_t)0x08000)
#define | EXTI_Line16 ((uint32_t)0x10000)
#define | EXTI_Line17 ((uint32_t)0x20000)
#define | EXTI_Line18 ((uint32_t)0x40000)
#define | IS_EXTI_LINE(LINE) ((((LINE) & (uint32_t)0xFFF00000) == 0x00) && ((LINE) != (uint16_t)0x00))
#define | IS_GET_EXTI_LINE(LINE)

## 枚举
enum | EXTIMode_TypeDef { EXTI_Mode_Interrupt = 0x00, EXTI_Mode_Event = 0x04 }
| EXTI mode enumeration 更多...
enum | EXTITrigger_TypeDef { EXTI_Trigger_Rising = 0x08, EXTI_Trigger_Falling = 0x0C, EXTI_Trigger_Rising_Falling = 0x10 }
| EXTI Trigger enumeration 更多...

## 函数
void | EXTI_DeInit (void)
| Deinitializes the EXTI peripheral registers to their default reset values. 更多...
void | EXTI_Init (EXTI_InitTypeDef *EXTI_InitStruct)
| Initializes the EXTI peripheral according to the specified parameters in the EXTI_InitStruct. 更多...
void | EXTI_StructInit (EXTI_InitTypeDef *EXTI_InitStruct)
| Fills each EXTI_InitStruct member with its reset value. 更多...
void | EXTI_GenerateSWInterrupt (uint32_t EXTI_Line)
| Generates a Software interrupt. 更多...
FlagStatus | EXTI_GetFlagStatus (uint32_t EXTI_Line)
| Checks whether the specified EXTI line flag is set or not. 更多...
void | EXTI_ClearFlag (uint32_t EXTI_Line)
| Clears the EXTI's line pending flags. 更多...
ITStatus | EXTI_GetITStatus (uint32_t EXTI_Line)
| Checks whether the specified EXTI line is asserted or not. 更多...
void | EXTI_ClearITPendingBit (uint32_t EXTI_Line)
| Clears the EXTI's line pending bits. 更多...

## 详细描述

This file contains all the functions prototypes for the EXTI firmware library.

作者
  megawin Application Team

版本
  V0.1.10

日期
  05-January-2023